{"text_format":"2","workbook":"xlsx","n_sheets":25,"sheets":["Cover","자가체크리스트","1. Applicant and facility Info","Checklist and Guideline","공정정보 작성 전 확인사항","1. 신청인 및 수소 생산설비 일반정보","2. 수소 생산공정 정보","Classification of Data","2.1. Natural Gas Prod.&Proc.","2.2. Feed Pre-treatment","2.3. Pre-reformer","2.4. Reformer(ATR, SMR, etc)","2.5. Water Gas Shift Reactor","2.6. CO2 Capture","2.7. Pressure Swing Adsorption","2.8. Compression (If nec.)","2.9. Air Separation Unit","2.10. CO2 Storage","2.11. Ind.&WasteTreat.(If nec.)","2.12. Other Utilities(If nec.)","3. Operating Conditions & Plan","4. Disclaimer","Q&A","Ecoinvent Index Method","데이터 코드 "],"not_rendered":{"charts":0,"images":13,"macros":0,"external_links":2,"defined_names":9,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":15,"n_cols":11,"rows_kept":15,"cut":false,"hidden":false,"merged":[[3,1,3,10],[2,2,2,10],[14,1,14,10],[11,1,11,10],[12,1,12,10],[7,1,9,10],[6,1,6,10]]}
[]
[]
[null,null,"Koreaˈs Clean Hydrogen Certification"]
[null,"  "]
[null,"  ","  ","  ","  ","  ","  ","  ","  ","  ","  "]
[{"$nulls":10},"  "]
[null,2025]
[null,"Application for Preliminary Review Consulting \non Clean Hydrogen Certification"]
[]
[]
[{"$nulls":10},"  "]
[]
[]
[null,null,"  ",null,"  "]
[null,"  "]

{"sheet":"자가체크리스트","index":1,"n_rows":35,"n_cols":4,"rows_kept":35,"cut":false,"hidden":true,"merged":[[1,1,1,2],[9,1,10,1]]}
[]
[null,"❚예비검토 컨설팅 참여를 위한 자가 체크리스트 "]
[]
[null,"점검항목","자가 점검 내용","체크박스 넣기"]
[null,"상세설계","단위 공정별 운전조건 및 물질흐름 등이 포함된 공정 흐름도(PFD)가 준비되고, 기술적 타당성 분석이 이루어졌는가? ","필수로 확인되어야하는 내용 위주로"]
[null,"상세설계","단위 공정별 투입물, 산출물이 정의되고 물지수지, 에너지수지가 작성되었는가?","없으면 인정 안해줄 것도 판단되도록"]
[null,"상세설계","단위 공정별 설비의 운전부하, 생산능력 및 소비전력 등을 포함하는 구체적인 규격과 제원이 확정되었는가? ","지금 검토 시점에서 필요한 내용만 남기고 다 없애고"]
[null,"상세설계","원료, 연료, 에너지, 유틸리티, 기타 투입물의 공급처(제조사명, 원산지 정보 등) 정보가 포함된 구매계획이 수립되었는가?",">>기입 여부확인도 하고, 세부 정보도 입력하도록"]
[null,"운영계획","다양한 에너지원의 전력을 사용하는 경우 전력 종류별 사용 비율이 포함된 설비 운영계획이 수립되었는가?"]
[null,"운영계획","수소 생산설비 운전 조건 변동요인을 파악하고 그 영향을 분석하였는가? "]
[null,null,"(계절 영향, 설비 노화, 원료 변경 등)"]
[null,"운영계획","원료 및 에너지 투입물의 공급 변동과 압력, 온도 등 운전 조건 변경을 고려한 수소 생산설비 운영계획이 수립되어 있는가?"]
[null,"MRV","수소 생산공정의 투입물‧산출물 데이터의 측정‧보고‧검증(MRV) 절차 및 방법이 수립되어 있는가?"]
[null,"MRV","데이터 모니터링 시스템 구축 및 프로그램 운영계획을 수립하고 있는가?"]
[null,"배출계수","기본 제공 데이터를 사용할 수 없는 경우 공인 데이터와 설계 데이터를 활용해 배출량을 산정하고, 산정 결과를 증명할 수 있는 자료를  갖추고 있는가?"]
[null,"배출계수","프로젝트 고유 배출계수 개발 관련 산정방법과 시료채취·분석 규격, 시험성적서 등의 증빙자료를 확보 또는 확보 가능한가?"]
[null,"신청서","위의 내용을 입증하기 위한 구체적인 증거 서류가 포함된 신청서를 작성하였는가?"]
[]
[]
[]
[null,"점검항목","자가 점검 내용","확인"]
[null,"충족 요건","CCS 공정에서의 CO2 포집율 90% 이상을 만족하는가?"]
[null,"충족 요건","수소제품의 순도 요건인 99%를 만족하는가?"]
[null,"양식 제출","SOR(Start of Run)과 EOR(End of Run) 기준의 투입-산출물 흐름 자료가 각각 제출 되는가?"]
[null,"자료제출","물질 수지 및 전과정평가를 위한 공정흐름도(PFD)가 제출 되는가?"]
[null,null,"프로젝트 진행 단계(EPC, FID, FEED, pre-FEED 등)"]
[null,null,"(해당시) PPA 사업 계획 수행 증빙 자료(LOI, MOU, HOA)"]
[null,null,"(해당시) 천연가스 업스트림 자료"]
[null,null,"(해당시) CCS 자료"]
[null,null,"운영계획의 구체성? >> 관련 제출 서류들"]
[null,null,"연간 수소 생산량 및 수출 계획 물량"]
[null,null,"수소 생산 개시 시점"]
[null,null,"'24 기지원 프로젝트에 대한 중복지원 여부"]
[null,null,"재무안전성 평가를 위한 기업 신용등급 결과를 작성 및 제출 하였는가?"]
[null,null,"지원 프로젝트에 한국 기업이 참여 여부를 작성하였는가?"]

{"sheet":"1. Applicant and facility Info","index":2,"n_rows":58,"n_cols":7,"rows_kept":58,"cut":false,"hidden":false,"merged":[[3,5,3,6],[38,2,40,3],[28,1,28,2],[24,1,24,2],[13,1,13,2],[27,1,27,2],[15,1,17,1],[28,3,28,6],[27,3,27,6],[31,1,37,1],[32,2,34,2],[29,1,30,1],[29,4,29,6],[25,1,25,2],[18,5,18,6],[19,5,19,6],[13,3,13,6],[43,2,44,6],[45,2,46,6],[40,5,40,6],[39,5,39,6],[37,3,37,5],[36,3,36,5],[35,3,35,5],[34,3,34,5],[33,3,33,5],[32,3,32,5],[31,2,31,5],[29,2,29,3],[35,2,37,2],[38,5,38,6],[38,4,40,4],[2,1,2,5],[3,1,3,2],[4,1,5,2],[4,3,5,3],[12,1,12,2],[6,1,11,1],[6,2,8,2],[10,3,10,6],[9,3,9,6],[11,3,11,6],[12,3,12,6],[8,3,8,6],[7,3,7,6],[6,3,6,6],[9,2,11,2],[4,5,5,6],[55,1,58,1],[55,2,56,2],[55,3,56,6],[57,2,58,2],[57,3,58,6],[47,2,48,2],[47,4,48,6],[38,1,40,1],[41,1,42,1],[49,2,50,6],[42,4,42,6],[42,2,42,3],[41,2,41,3],[41,4,41,6],[15,5,15,6],[30,2,30,6],[23,1,23,5],[26,3,26,6],[24,5,24,6],[17,5,17,6],[18,1,18,2],[16,5,16,6],[20,5,20,6],[19,3,20,3],[19,1,20,2],[26,1,26,2],[25,3,25,6],[21,1,21,3],[21,4,21,6],[53,1,54,1],[53,3,54,3],[4,4,5,4],[49,1,50,1],[45,1,46,1],[47,1,48,1],[51,1,52,1],[51,3,52,3],[14,1,14,2],[14,3,14,6],[51,2,52,2],[53,2,54,2],[53,4,54,6],[51,6,52,6],[51,5,52,5],[51,4,52,4]]}
[]
[null,"1. Applicant and Hydrogen Production Facility Information"]
[null,"❚Applicant General information"]
[null,"Trade name (Entity name)",null,"OOOO","Business registration number","  000-00-00000"]
[null,"Representative name",null,"OOOO","Date of Birth\n(Corporation registration no.)","000000-00000000"]
[]
[null,"Location","HQ","Address: "]
[null,null,null,"(Tel.: ) +00-0000-0000"]
[null,null,null,"(Fax: ) "]
[null,null,"Manufacturing Plant","Address: "]
[null,null,null,"(Tel.: ) +00-0000-0000"]
[null,null,null,"(Fax: ) "]
[null,"Corporate Credit Rating Results",null,"Select from [AA-or higher / A+~A- / BBB+~BB- / B+ or lower]\n\n※ Enter the credit rating of the hydrogen production company for the project\n- If the two or more companies participate the project, or \nif the hydrogen production company is a newly established company founded within 9 years of the applicant deadline, \nthe credit rating result of the largest shareholder(Excluding financial institutions) of the project may be submitted."]
[null,"Participation of Korean Companies",null,"Select from [Direct development / Equity investment / Off-taking / Non-participation] "]
[null,"Business Structure",null,"A company / Shareholding ratio 50%\nB company / Shareholding ratio 30%\nC company / Shareholding ratio 20%"]
[null,"Contact Point","Team",null,"Name","O O O"]
[null,null,"Position",null,"E-mail","abc@ooo.com"]
[null,null,"Contact No.","010-0000-0000,  \n02-0000-0000","FAX","010-0000-0000,  \n02-0000-0000"]
[null,"CHPS Bid Participation Year",null,"'25 or '26"]
[null,"Preliminary Review Consulting Participation Record",null,"O/X","Modifications Compared to '24\n(If applicable)","Select from [Major modification / Minor modification / No modification]"]
[{"$nulls":4},"Modification Details"]
[{"$nulls":4},"※ Major modifications\n - Modification of fuel/raw procurement plans\n(Example : Changes in the natural gas field, fluctuations in PPA contracts affecting grid electricity proportion, modifications in water supply methods related to the changes in power supply methods)\n - Change of CO2 storage sites\n - Other factors affecting the preliminary review consulting results from '24"]
[]
[null,"❚Hydrogen Production Facility Information"]
[null,"Project name",null,null,"Project Status","Select from [Under construction or FID / FEED or pre-FEED / FS / pre-FS]"]
[null,"Expected date of completion"]
[null,"Expected date of operation"]
[null,"Location of the facility",null,"(Address)"]
[null,"Major facilities"]
[null,"Method of Hydrogen production","□ Natural gas steam reforming (with CCS) ",null,"□ Natural gas autothermal reforming (with CCS)"]
[null,null,"□ Other (                                    )"]
[null,"Source of Energy ","Category",null,null,null,"Ratio(%)"]
[null,null,"Electricity","Renewable energy (□ Solar power, □ Wind power, \n□ Hydro power, □ Other [ ])",null,null,"  "]
[null,null,null,"National grid (Grid country : )"]
[null,null,null,"Other (planning to use low-carbon energy source via eligible PPA)"]
[null,null,"Heat","Fossil fuels (□ coal, □ NG, □ Others [ ])",null,null,"  "]
[null,null,null,"Non-fossil fuels (source:                                  )",null,null,"  "]
[null,null,null,"Other (                                               )",null,null,"  "]
[null,"Natural Gas procurement source","Direct supply from specific gas field / \nDemand from the natural gas supply chane",null,"Type of gas field","conventional / unconventional"]
[{"$nulls":5},"associated / non-associated"]
[{"$nulls":5},"On shore / Off shore"]
[null,"Utility and \nother input materials","□ Heat(steam) \n(□internal production □external purchase)",null,"□ Process water"]
[null,null,"□ Compressed air",null,"□ Other (                                      )"]
[null,"Facility production capacity","100,000 TPY"]
[null,"(TPY)"]
[null,"Annual operation rate (% or hr)","91% / 8000 hr"]
[]
[null,"Hydrogen product purity (vol%)",0.999,"Impurity","CO 0.05%, N2 0.05%"]
[null,null,null,"(each impurity type and vol%)"]
[null,"Hydrogen product pressure (bar)"]
[]
[null,"CO2 capture (Y / N)",null,"CO2 capture capacity (kgCO2/hr)",null,"CO2 capture rate (%)"]
[]
[null,"CO2 storage (Y / N)",null,"CO2 storage capacity (kgCO2/hr)"]
[]
[null,"Details on CO2 storage and transportation","CO2 storage countries","ex) US/ AUS ETC…"]
[]
[null,null,"CO2 transportation and distance information","ex)US XXGas field (an area 100 km off the northern coast)\nShipping Trasportation 800km"]

{"sheet":"Checklist and Guideline","index":3,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[[14,4,14,5],[15,1,16,1],[16,4,16,5],[17,4,17,5],[18,1,19,1],[18,4,18,5],[19,4,19,5],[1,1,1,3],[6,1,6,2],[12,1,13,1],[13,4,13,5],[7,1,11,1],[9,2,11,2],[4,2,4,3],[5,2,5,3],[20,1,21,1],[23,1,23,3],[25,1,25,2],[25,4,25,5],[26,1,26,2],[26,4,26,5],[27,1,27,2],[27,4,27,5],[28,1,28,2],[28,4,28,5],[29,1,29,2],[29,4,29,5],[30,1,30,2],[30,4,30,5],[32,1,32,3],[34,1,34,2],[34,3,34,5],[35,1,35,2],[35,3,35,5],[36,1,40,1],[36,3,36,5],[37,3,37,5],[38,3,38,5],[39,3,39,5],[40,3,40,5]]}
[]
[null,"❚Submission and Completion of Mandatory Items"]
[null,null,"※ The file name of the submitted supporting documents must start with the [document submission number], \n"]
[null,null,"    and the documents should be submitted as a single compressed file (.zip)"]
[null,null,"Example)\n   [1-1] Company name_Hydrogen Production PFD_01.pdf , [1-2] Company name_Hydrogen Production PFD_02.pdf\n   [2] Company name_SOR Applicantion Form.xlsx"]
[]
[null,"Checklist items",null,"Content","YES","NO","Submission Number"]
[null,"Consulting Eligibility","Eligible pathway","The CO2 capture rate exceeds 90% in the case of reforming hydrogen + CCS",null,null,"-"]
[null,null,"Purity requirement","Hydrogen product meets the purity requirement of 99% or higher",null,null,"-"]
[null,null,"Submission of basic data","Submission of data above PFD level for mass balance verification\n * Documents written in English or Korean\n * Documents with sufficient resolution for data identification",null,null,"[1]"]
[null,null,null,"A separate excel form based on SOR(Start of Run) is prepared and submitted",null,null,"[2]"]
[null,null,null,"A separate excel form based on EOR(End of Run) is prepared and submitted",null,null,"[3]"]
[null,"Business Credibility","Submission status","Submission of credit rating report",null,null,"[4]"]
[null,null,"Credit rating","Select from [AA- or above / A+ to A- / BBB+ to BB- / B+ or below]",null,null,"-"]
[null,"Participation of Korean Companies","Shareholding structure","Select from [Direct development / Equity investment / Off-taking / Non-participation] ",null,null,"[5]"]
[null,"Previous year Preliminary Review Consulting","Participation record","Participation history of preliminary review consulting of the same project in the previous year",null,null,"-"]
[null,null,"Modification Details","Select from [Not applicable / Major modification / Minor modification / No modification]",null,null,"-"]
[null,"Business Plan Specificity","Project implementation stage","Select from [Under construction or FID / FEED or pre-FEED / FS / pre-FS]",null,null,"-"]
[null,"Plant Capacity and Timeline","Hydrogen production capacity","Described the annual hydrogen production capacity and planned export quantitiy to Korea\n(Unit: TPY)",null,null,"-"]
[null,null,"Expected date of operation","Select from [2028 / 2029 / After 2030]",null,null,"-"]
[null,"Feasibility of Business Plan","NG Upstream","The emissions for upstream of natural gas process are reported\n(Whether '2.1. Natural Gas Prod.&Proc.' sheet is prepared)",null,null,"[6]"]
[null,null,"CCS","The documents to prove the feasibility of the CCS operation plan are submitted\n - Supporting documents for CCS storage site permitting\n - Review materials to ensure CCS operational stability\n - Monitoring methodology and plans, etc.",null,null,"[7]"]
[]
[null,"❚ Applicant Document Input Data Self-Checklist"]
[]
[null,"Category",null,"Content","Check"]
[null,"Data input units",null,"Has the unit for mass flow [kg/hr] and energy flow [kWh/hr] been followed?","[YES / NO]"]
[null,"Material and energy balace",null,"Does the material and energy balance for each unit process meet the allowed error range of 0.01%?","[YES / NO]"]
[null,"Significant figures of input data",null,"Has the significant figures been applied up to the fourth decimal place?","[YES / NO]"]
[null,"Other chemical substance information input",null,"Has the information for catalyst and other chemicals been entered considering usage and loss, calculated as the annual average usage?","[YES / NO]"]
[null,"Production plan information input",null,"Has \"3. Operating conditions and production plan\" been documented regarding the material and energy flows entering and exiting the overall system boundary?","[YES / NO]"]
[]
[null,"❚ Process information writing guidelines"]
[]
[null,"Category",null,"Content"]
[null,"Unit process classification",null,"ㅇ Feedstock Treatment\n  - Fired Heater\n  - Pre-treatment\n  - Pre-reformer\nㅇ Hydrogen Production\n  - Reformer\n  - Water Gas Shift reactor\n  - Hydrogen Purification (PSA)\n  - Hydrogen Compression\nㅇ Carbon Capture and Storage\n  - Carbon Capture Process\n  - Captured Carbon Storage\nㅇ Utility\n\n* Additional processes can be added depending on the facility configuration"]
[null,"Entering unit process data","Common","ㅇ Input data unit : All data should be written using the time unit of hr\n  - Material flow is based on mass flow, with units in kg/hr\n  - Energy flow should be represented in kWh/hr\nㅇ For material streams, quantity, density and composition data is required\n  - Composition should be given in mol%, and the total must sum to 100%\nㅇ The stream between unit processes should be linked using Excel formulas, and the connection information should be recorded as follows:\n  - From outside the system boundary / To outside the system boundary\n  - From Sheet No.(2.X)-Out-Sheet No. / To Sheet No.(2.X)-In-Sheet No.\n   (e.g., From 2.2-Out-8)\n  - If not applicable, provide a detailed explanation\nㅇ Check the material and energy balance of the unit process is satisfied (Tolerance range : < 0.01%)\nㅇ Steam flow informaton requires temperature(°C) and pressure(bar) input\nㅇ The treatment process for waste flow in the unit process needs to be specified\nㅇ Information on catalysts and chemical products(material name, usage, detailed composittion, etc.) should be provided\n  - CAS No. is required for chemicals\n  - The usage amount should be converted to the annual average usage amount, considering the replacement cycle, loss amount, etc"]
[null,null,"Feedstock\nTreatment","ㅇ Fired Heater exhaust gas and waste flow documentation required\nㅇ Check whether utility flow information for heat recovery is indicated\nㅇ For fuel and raw materials, detailed composition should be provided to match the specified heating value provided"]
[null,null,"Hydrogen\nProduction","ㅇ When pure oxygen is used in the process, the source information needs to be checked\n  - If purchased externally, check the supplier information and power consumption\n  - If produced internally, an ASU sheet needs to be added individually\nㅇ In hydrogen compression, the final discharge pressure of hydrogen should be recorded\nㅇ Check whether utility flow information for heat recovery is indicated"]
[null,null,"Carbon Capture and Storage","ㅇ If it is possible to enter detailed information (CO2 temperature, pressure conditions, phase, transportation distance, etc.) according to the detailed steps of CCS, such as \"compression\", \"pipeline transportation\", and \"injection\", please provide detailed information\nㅇ Check whether the transportation distance between the capture process and the storage site is recorded\nㅇ Check whether the leakage amount during the CO2 transportation process is provided\nㅇ Check whether information on the auxiliary facilities required for the CO2 storage process (e.g., compressors) and utility usage is provided"]
[null,null,"Utility","ㅇ Check whether the boiler feed water and steam stream data between unit processes are provided\nㅇ The entry and exit stream at the system boundary(BFW, Make-up, Steam product) should be clearly defined\nㅇ If the ASU is included within the battery limit, it should be written as a separate unit process\nㅇ The power generation amount in the respective system should to be recorded when building a power generation system"]

{"sheet":"공정정보 작성 전 확인사항","index":4,"n_rows":12,"n_cols":4,"rows_kept":12,"cut":false,"hidden":true,"merged":[[7,1,11,1],[1,1,1,3],[6,1,6,2],[5,1,5,2],[4,1,4,2],[3,1,3,2]]}
[]
[null,"❚공정정보 작성 가이드라인"]
[]
[null,"점검항목",null,"확인 내용"]
[null,"자료 제출",null,"ㅇ각 설비의 SOR(Start of Run)과 EOR(End of Run) 수치를 별도의 엑셀파일로 제공 필요\nㅇ 전력/천연가스/CCS 자료제출"]
[null,"신청양식 작성",null,"ㅇ '신청인 및 수소 생산설비 일반정보'와 '수소 생산공정 정보' 필수 작성\nㅇ 천연가스의 업스트림 배출량 산정을 위해 '천연가스 생산 및 조달 계획' 시트 작성\nㅇ 2.X 시트는 단위공정 기준의 물질 및 에너지 수지 정보를 기입하며, 이를 바탕으로 '4. 운전 조건 및 생산계획' 시트에서는 시스템경계를 출입하는 투입물과 산출물만을 기입"]
[null,"단위 공정\n구분",null,"ㅇ Feedstock Treatment\n - Fired Heater\n - Pre-treatment\n - Pre-reformer\nㅇ Hydrogen Production\n - Reformer\n - Water Gas Shift reactor\n - Hydrogen Purification (PSA)\n - Hydrogen Compression\nㅇ Carbon Capture and Storage\n - Carbon Capture Process\n - Captured Carbon Storage\nㅇ Utility\n - Air Separation Unit\n - Steam Cycle"]
[null,"단위 공정\n정보 입력","공통","ㅇ 데이터 입력 단위 : 모든 데이터의 시간 단위는 hr를 기준으로 작성\n - 물질 흐름은 질량 흐름을 기준으로 하며, 단위는 kg/hr 적용\n - 에너지 흐름은 kWh/hr 단위로 표기\nㅇ 모든 데이터의 유효숫자는 소수점 넷째 자리까지 하여 입력\nㅇ 물질 흐름에 대한 양, 밀도, 조성 입력 필요\n - 조성은 mol%를 기준으로 입력하며, 총 합이 100%가 되도록 기재\n - 정확한 조성의 입력이 필요하며, Cn+로 표기되는 탄화수소 화합물의 경우, 물질 수지를 고려하여 대표물질 입력 및 *표기\n   (e.g., [CH4 95%, C2+ 5%] >> [CH4 95%, *C3H8 5%])\nㅇ 단위 공정 사이의 흐름에 대해서는 엑셀의 수식 기능을 활용하여 연계하고, 연결 정보를 아래와 같이 기재\n - From 시스템 경계 밖 / To 시스템 경계 밖\n - From 시트 번호(2.X)-Out-번호 / To 시트번호(2.X)-In-번호\n   (e.g., From 2.2-Out-8)\n - 위에 해당하지 않는 경우, 자세한 설명 기재\nㅇ 단위 공정별 물질 및 에너지 수지 확인 (오차범위 0.01% 이내)\nㅇ 단위 공정 내 폐기물 흐름의 처리 과정 기입 필요\nㅇ 촉매 및 화학제품에 대한 정보 (물질명, 교체 주기, 사용량 등) 기입 필요\n - 화학물질은 CAS No. 기재\n - 사용량은 교체 주기, 손실량 등을 고려하여 연평균 사용량으로 환산하여 기재"]
[null,null,"Feedstock\nTreatment","ㅇ Fired Heater 배가스 및 폐기물 흐름 작성 필요\nㅇ 열회수를 위한 유틸리티 흐름 정보 확인\n - Utility 페이지와 흐름 연결 확인"]
[null,null,"Hydrogen\nProduction","ㅇ 순산소 사용 시 출처 확인 필요\n - 외부 구입 시, 구입처 정보 및 전력 소모량 확인 / 내부 생산 시, ASU 시트 작성 필요\nㅇ Hydrogen Compression에서는 수소 최종 토출 압력 기재\nㅇ 열회수를 위한 유틸리티 흐름 정보 확인\n - Utility 페이지와 'From', 'To' 매칭"]
[null,null,"Carbon Capture and Storage","ㅇCCS의 세부적인 단계인 '압축', '파이프라인 운송', '주입' 의 단계에 따라 자세한 정보들\n   (CO2의 온도, 압력, 농도 조건, 상(phase), 운송거리 등)의 기입이 가능하면, 세부적인 정보 제공이 필요\nㅇ 포집 공정과 저장소 사이의 운송 거리 기재 확인\nㅇ 이산화탄소 운송 과정 중 누출량 정보 확인\nㅇ 이산화탄소 저장 과정에서 요구되는 부대 설비의 정보(예: 압축기)와 유틸리티 사용량 확인"]
[null,null,"Utility","ㅇ 단위공정간 보일러수 및 스팀 흐름 정보 확인\nㅇ 시스템 경계 출입 흐름(BFW, Makeup, Steam product) 정보 명확하게 작성 필요\nㅇ 공정 경계 내 ASU 포함 시, 별도 단위 공정으로 작성 필요\nㅇ 발전 시스템 구축 시, 해당 시스템에서의 발전량 기입 필요"]

{"sheet":"1. 신청인 및 수소 생산설비 일반정보","index":5,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":true,"merged":[[11,3,11,5],[12,3,12,5],[16,1,16,2],[13,1,15,1],[2,1,2,5],[3,1,3,5],[4,1,4,2],[5,1,6,2],[5,3,6,3],[5,5,6,5],[7,1,12,1],[7,2,9,2],[7,3,7,5],[8,3,8,5],[9,3,9,5],[10,3,10,5],[20,1,20,2],[20,3,20,5],[17,1,18,2],[17,3,17,4],[19,1,19,2],[21,1,21,2],[21,3,21,5],[22,1,22,2],[22,3,22,5],[33,2,33,4],[23,1,23,2],[23,3,23,5],[26,1,26,5],[27,1,27,5],[28,2,28,4],[29,2,29,4],[29,5,33,5],[30,2,30,4],[31,2,31,4],[32,2,32,4]]}
[]
[null,"1. 신청인 및 수소 생산설비 일반정보"]
[null,"1.1. 신청인 및 수소 생산설비 일반정보"]
[null,"❚신청인 일반정보"]
[null,"상호(법인명)",null,"OOOO","사업자등록번호","  000-00-00000"]
[null,"대표자성명 ",null,"OOOO","생년월일","000000-00000000"]
[{"$nulls":4},"(법인등록번호)"]
[null,"소재지","본사","주소: "]
[null,null,null,"(전화: ) 02-0000-0000"]
[null,null,null,"(팩스: ) 02-0000-0000"]
[null,null,"제조","주소: "]
[null,null,"공장","(전화: ) 02-0000-0000"]
[null,null,null,"(팩스: ) 02-0000-0000"]
[null,"담당자","소속","청정수소팀","성명","O O O"]
[null,null,"직위","팀장","전자우편","abc@ooo.com"]
[null,null,"연락처","010-0000-0000,  \n02-0000-0000","팩스","02-0000-0000"]
[null,"CHPS 입찰참가연도",null,"'24 or '25"]
[null,"설비유형\n(선택 및 기입)",null,"[□]SMR+연소전·후 탄소포집률(  %)",null,"[□]SMR+연소전 탄소포집률(  %)"]
[null,null,null,"[□]ATR+탄소포집률(  %)","[□] 수전해 [       ]","[□] 기타 [                   ] "]
[null,"프로젝트명",null,null,"프로젝트 진행단계"]
[null,"준공예정일",null,"ㄴㅇㄻㄴㅇㄹ"]
[null,"운영예정일"]
[null,"설비소재지",null,"(도로명 주소)"]
[null,"주요설비"]
[null,"* 컨설팅 수요가 예상치를 초과시, 입찰참가 시기의 시급성 및 프로젝트 개발의 구체성을 기반으로 선정 예정"]
[]
[null,"1.2. 수소 생산설비 정보"]
[null,"❚수소 생산설비 일반정보"]
[null,"항목","내용",null,null,"생산 설비 전경"]
[null,"시설명","SMR/ATR 프로젝트"]
[null,"준공일","0000. 00. 00 (준공 이전일 경우 예정일)"]
[null,"운영시작일","2023. 12. 00 (운영 이전일 경우 예정일)"]
[null,"소재지","OOOO "]
[null,"주요시설"]

{"sheet":"2. 수소 생산공정 정보","index":6,"n_rows":44,"n_cols":6,"rows_kept":44,"cut":false,"hidden":true,"merged":[[30,1,33,1],[35,1,48,1],[35,4,35,5],[13,2,13,3],[13,4,13,5],[15,1,17,1],[15,2,15,3],[15,4,15,5],[16,2,16,3],[16,4,16,5],[17,2,17,3],[17,4,17,5],[34,2,34,5],[14,2,14,3],[14,4,14,5],[18,2,19,5],[48,4,48,5],[1,1,1,5],[9,3,9,4],[10,2,12,2],[3,1,5,1],[3,2,3,3],[3,4,3,5],[5,2,5,3],[5,4,5,5],[6,1,12,1],[6,2,6,4],[7,2,9,2],[7,3,7,4],[8,3,8,4],[10,3,10,4],[11,3,11,4],[20,2,21,5],[30,3,31,5],[28,4,29,5],[26,4,27,5],[24,2,25,5],[28,2,29,2],[26,2,27,2],[22,2,23,2],[22,4,23,5],[4,4,4,5],[4,2,4,3],[32,3,33,5],[46,4,46,5],[47,4,47,5],[36,4,36,5],[37,4,37,5],[38,4,38,5],[39,4,39,5],[40,4,40,5],[41,4,41,5],[42,4,42,5],[43,4,43,5],[44,4,44,5],[45,4,45,5],[12,3,12,4]]}
[]
[null,"2. 수소 생산공정 정보"]
[]
[null,"① 수소 생산방식","□ 수전해(수전해타입: Alkaline)",null,"□ 수전해(수전해타입: PEM)"]
[null,null,"□ 수전해(수전해타입: SOEC 등)",null,"■ 천연가스 수소생산 스팀개질법(CCS 포함) "]
[null,null,"□ 천연가스 자열개질법(CCS 포함) ",null,"□ 기타 ( )"]
[null,"② 에너지원","구분",null,null,"비율(%)"]
[null,null,"전기에너지","재생에너지 (□ 태양광, □ 풍력, □ 수력, □ 기타 [ ])",null,"  "]
[null,null,null,"국가전력망 ",null,"0~20"]
[null,null,null,"기타 ( PPA 계약을 통한 저탄소 에너지원 사용 예정 )",null,"80~100"]
[null,null,"열에너지","화석연료 (□ 석탄, □ LNG, □ 기타 [ ])",null,"  "]
[null,null,null,"비화석연료 (source:                       )",null,"  "]
[null,null,null,"기타 (                        )",null,"  "]
[null,"유틸리티 및 ","■열(스팀) (■내부생산 □외부구매)",null,"■ 공정수"]
[null,"기타투입물 현황","□압축공기",null,"□ 기타 ( )"]
[null,"③ 가동상황","■완전 정상 가동상태",null,"□부분 정상 가동상태"]
[null,null,"□파일럿 단계",null,"□실험 단계"]
[null,null,"□미가동 (가동예정:             년도)",null,"□기타 ( )"]
[null,"④ 시설 생산용량","100,000 TPY"]
[null,"(TPY)"]
[null,"⑤ 연간 공정 가동률","91% / 8000 hr"]
[null,"(% or hr)"]
[null,"⑥ 수소 제품 순도",0.999,"불순물","CO 0.05%, N2 0.05%"]
[null,"(vol%)",null,"(각 불순물 종류 및 vol%)"]
[null,"⑦ 수소 제품 압력"]
[null,"(bar)"]
[null,"⑧ 이산화탄소 포집",null,"이산화탄소 포집 용량"]
[null,"여부 (예/아니오)",null,"(kgCO2/hr)"]
[null,"⑨ 이산화탄소 저장",null,"이산화탄소 저장 용량"]
[null,"여부 (예/아니오)",null,"(kgCO2/hr)"]
[null,"⑩ 이산화탄소 저장 및 운송 관련 세부사항 ","이산화탄소","ex)호주"]
[null,null,"저장 국가"]
[null,null,"이산화탄소","ex)북호주 XX가스전 (YY 북부 100 km 해상), 선박 운송 800km"]
[null,null,"운송 수단 및 거리 정보"]
[null,"⑪ 공정흐름도","\n\n\n\n\n\n\n\n\n\n\n\n공정 운전조건 (예: 온도, 압력, 유량, 조성 등)을 알 수 있는 공정 흐름이 포함된 공정흐름도. \n단위공정별 고유번호(흐름 순서) 표기, 생산 공정 정보표와 일치하도록 작성"]
[null,"⑫ 단위설비설명","단위설비명","단위 공정 흐름도","설비설명(예)"]
[null,null,"Feed Pre-treatment/Fired heater",null,"- 전처리 반응기에서 원료에 포함된 sulfur 성분 제거"]
[null,null,"Pre-reformer",null,"-  원료 내 CH4보다 무거운 탄화수소를 steam과 반응시켜 CH4, H2로 개질"]
[null,null,"Autothermal reformer",null,"- 순산소(O2) 주입을 통해 순산소와 혼합가스를 반응시켜 개질가스(H2, CO, CO2)를 생성"]
[null,null,"Water Shift reactor",null,"- 스팀을 주입하여 개질가스 내의 CO와 반응시켜 H2 및 CO2를 생산"]
[null,null,"CO2 Capture\n(CCP)",null,"- Amine 수용액을 흡수제로 이용하여 개질가스 중 CO2를 흡수하여 포집"]
[null,null,"PSA",null,"- 흡착/감압/재생/압축 단계를 거쳐 99 vol%의 H2를 생산"]
[null,null,"CCS",null,"-포집된 CO2의 저장지 주입까지의 공정"]
[null,null,"Steam System",null,"-공정 내 열에너지 활용을 위한 스팀 생산 및 스팀 터빈을 통한 소내 발전"]

{"sheet":"Classification of Data","index":7,"n_rows":84,"n_cols":5,"rows_kept":84,"cut":false,"hidden":false,"merged":[[54,2,56,2],[6,2,13,2],[14,2,18,2],[19,2,21,2],[22,2,25,2],[32,2,35,2],[36,2,38,2],[39,2,41,2],[42,2,44,2],[45,2,47,2],[48,2,50,2],[51,2,53,2],[57,2,62,2],[63,2,67,2],[68,2,70,2],[71,2,77,2],[78,2,83,2]]}
[]
[]
[null,null,"Classification of Input-Output data"]
[]
[null,null,"<Main category>"]
[null,null,"Item","Main category","Details"]
[null,null,"Fuel","Fuel for raw material production facility for hydrogen production","Example) Fuel for pure water production facility"]
[null,null,null,"Main fuel for hydrogen production facilities","Example) NG for Steam reforming reactor"]
[null,null,null,"Auxiliary fuel for hydrogen production facilities"]
[null,null,null,"Fuel for power generation facility"]
[null,null,null,"Fuel for heat production facilty"]
[null,null,null,"Fuel for other utility facilty"]
[null,null,null,"Fuel for other transportation facilities (including mobile combustion)"]
[null,null,null,"Other fuels"]
[null,null,"Raw Material","Raw material for hydrogen production"]
[null,null,null,"Raw material for producing products other than hydrogen"]
[null,null,null,"Heat"]
[null,null,null,"Electricity"]
[null,null,null,"Other raw materials"]
[null,null,"Input Material","Catalyst"]
[null,null,null,"Reducing agent"]
[null,null,null,"Other input materials"]
[null,null,"Output Material","Hydrogen"]
[null,null,null,"By-products(carbon-containing)"]
[null,null,null,"By-products(carbon-free)"]
[null,null,null,"Other by-products"]
[null,null,"Waste","Waste"]
[]
[]
[null,null,"<Middle category and subcategory>"]
[null,null,"Middle category","Subcategory","Explanation"]
[null,null,"Hydrogen","Hydrogen"]
[null,null,"Natural Gas","Domestic city gas","City gas in Korea considering NG import ratio"]
[null,null,null,"Imported natural gas","NG produced overseas, imported to Korea and use in Korea"]
[null,null,null,"Foreign city gas","Overseas city gas (average natural gas in the country) produced and used locally"]
[null,null,null,"Overseas city gas","Overseas natural gas (individual gas field) production, local use"]
[null,null,"Bituminous Coal","Domestic bituminous coal","Bituminous coal in Korea considering the bituminous coal import ratio"]
[null,null,null,"Imported bituminous coal","Bituminous coal produced overseas, imported to Korea and use in Korea"]
[null,null,null,"Overseas bituminous coal","Overseas bituminous coal production, local use"]
[null,null,"Anthracite","Domestic anthracite","Anthracite in Korea considering anthracite import ratio"]
[null,null,null,"Imported anthracite","Anthracite produced overseas, imported to Korea and use in Korea"]
[null,null,null,"Overseas anthracite","Overseas anthracite production, local use"]
[null,null,"LPG\n(liquefied petroleum gas)","Domestic LPG","LPG in Korea considering LPG import ratio"]
[null,null,null,"Imported LPG","LPG produced overseas, imported to Korea and use in Korea"]
[null,null,null,"Overseas LPG","Overseas LPG production, local use"]
[null,null,"Propane","Domestic propane","Propane produced at a refinery in Korea"]
[null,null,null,"Imported propane","Propane produced overseas, imported to Korea and use in Korea"]
[null,null,null,"Overseas propane","Overseas propane production, local use"]
[null,null,"Heavy Oil\n(Bunker C oil)","Dometic Bunker C oil","Bunker C oil produced at a refinery in Korea"]
[null,null,null,"Imported Bunker C oil","Bunker C oil produced overseas, imported to Korea and use in Korea"]
[null,null,null,"Overseas Bunker C oil","Overseas bunker C oil production, local us"]
[null,null,"Light Oil","Domestic light oil","Light oil produced at a refinery in Korea"]
[null,null,null,"Imported light oil","Light oil produced overseas, imported to Korea and use in Korea"]
[null,null,null,"Overseas light oil","Overseas light oil production, local use"]
[null,null,"Gasoline","Domestic gasoline","Gasoline produced at a refinery in Korea"]
[null,null,null,"Imported gasoline","Gasoline produced overseas, imported to Korea and use in Korea"]
[null,null,null,"Overseas gasoline","Overseas gasoline production, local use"]
[null,null,"Electricity","Grid electricity"]
[null,null,null,"Renewable electricity(Solar)"]
[null,null,null,"Renewable electricity(Wind)"]
[null,null,null,"Renewable electricity(Hydro power)"]
[null,null,null,"Nuclear electricity"]
[null,null,null,"Other electricity"]
[null,null,"Heat","Heat(Steam, based on natural gas boiler)"]
[null,null,null,"Heat(Steam, based on combined heat and power plant)"]
[null,null,null,"Heat(Steam, based on other fuel)"]
[null,null,null,"Heat (Hot water)"]
[null,null,null,"Heat (Other)"]
[null,null,"Common","Pure water"]
[null,null,null,"Industrial water"]
[null,null,null,"Other"]
[null,null,"Chemical Substance","Hydrogen chloride(HCl) Solution"]
[null,null,null,"Sodium hydroxide(NaOH) Solution"]
[null,null,null,"Potassium hydroxide (KOH) Solution"]
[null,null,null,"CO2 absorbent (MEA)"]
[null,null,null,"Oxygen(O2)"]
[null,null,null,"Nitrogen(N2)"]
[null,null,null,"Other"]
[null,null,"Other","Other solid fuel"]
[null,null,null,"Other liquid fuel"]
[null,null,null,"Other gas fuel"]
[null,null,null,"Other solid non-fuel"]
[null,null,null,"Other liquid non-fuel"]
[null,null,null,"Other gas non-fuel"]

{"sheet":"2.1. Natural Gas Prod.&Proc.","index":8,"n_rows":194,"n_cols":37,"rows_kept":194,"cut":false,"hidden":false,"merged":[[188,28,190,28],[188,29,190,29],[188,30,190,30],[188,31,190,31],[189,11,189,14],[190,11,190,14],[188,22,190,22],[188,23,190,23],[188,24,190,24],[188,25,190,25],[188,26,190,26],[188,27,190,27],[188,16,190,16],[188,17,190,17],[188,18,190,18],[188,19,190,19],[188,20,190,20],[188,21,190,21],[186,1,190,2],[186,3,190,4],[186,5,187,6],[186,7,187,10],[186,11,186,14],[187,11,187,14],[188,5,190,6],[188,7,190,10],[188,11,188,14],[180,29,185,29],[180,30,185,30],[180,31,185,31],[181,11,181,14],[182,11,182,14],[183,11,183,14],[184,11,184,14],[185,11,185,14],[180,23,185,23],[180,24,185,24],[180,25,185,25],[180,26,185,26],[180,27,185,27],[180,28,185,28],[180,17,185,17],[180,18,185,18],[180,19,185,19],[180,20,185,20],[180,21,185,21],[180,22,185,22],[180,1,185,2],[180,3,185,4],[180,5,185,6],[180,7,185,10],[180,11,180,14],[180,16,185,16],[175,29,177,29],[175,30,177,30],[175,31,177,31],[176,11,176,14],[177,11,177,14],[178,3,179,4],[178,5,179,6],[178,7,179,10],[178,11,178,14],[179,11,179,14],[175,23,177,23],[175,24,177,24],[175,25,177,25],[175,26,177,26],[175,27,177,27],[175,28,177,28],[175,17,177,17],[175,18,177,18],[175,19,177,19],[175,20,177,20],[175,21,177,21],[175,22,177,22],[172,30,174,30],[172,31,174,31],[173,11,173,14],[174,11,174,14],[175,1,179,2],[175,3,177,4],[175,5,177,6],[175,7,177,10],[175,11,175,14],[175,16,177,16],[172,24,174,24],[172,25,174,25],[172,26,174,26],[172,27,174,27],[172,28,174,28],[172,29,174,29],[172,18,174,18],[172,19,174,19],[172,20,174,20],[172,21,174,21],[172,22,174,22],[172,23,174,23],[172,3,174,4],[172,5,174,6],[172,7,174,10],[172,11,172,14],[172,16,174,16],[172,17,174,17],[166,30,167,30],[166,31,167,31],[167,11,167,14],[168,11,168,14],[169,11,169,14],[170,11,170,14],[166,24,167,24],[166,25,167,25],[166,26,167,26],[166,27,167,27],[166,28,167,28],[166,29,167,29],[166,18,167,18],[166,19,167,19],[166,20,167,20],[166,21,167,21],[166,22,167,22],[166,23,167,23],[162,29,165,29],[162,30,165,30],[162,31,165,31],[163,11,163,14],[164,11,164,14],[165,11,165,14],[162,22,165,22],[162,23,165,23],[162,24,165,24],[162,25,165,25],[162,26,165,26],[162,27,165,27],[162,16,165,16],[162,17,165,17],[162,18,165,18],[162,19,165,19],[162,20,165,20],[162,21,165,21],[161,11,161,14],[162,1,174,2],[162,3,165,4],[162,5,165,6],[162,7,165,10],[162,11,162,14],[159,23,161,23],[159,24,161,24],[159,25,161,25],[159,26,161,26],[159,27,161,27],[159,28,161,28],[159,17,161,17],[159,18,161,18],[159,19,161,19],[159,20,161,20],[159,21,161,21],[159,22,161,22],[166,3,171,4],[166,5,171,6],[166,7,171,10],[166,11,166,14],[166,16,167,16],[166,17,167,17],[171,11,171,14],[162,28,165,28],[157,29,158,29],[157,30,158,30],[157,31,158,31],[158,11,158,14],[159,1,161,2],[159,3,161,4],[159,5,161,6],[159,7,161,10],[159,11,159,14],[159,16,161,16],[157,23,158,23],[157,24,158,24],[157,25,158,25],[157,26,158,26],[157,27,158,27],[157,28,158,28],[157,17,158,17],[157,18,158,18],[157,19,158,19],[157,20,158,20],[157,21,158,21],[157,22,158,22],[157,1,158,2],[157,3,158,4],[157,5,158,6],[157,7,158,10],[157,11,157,14],[157,16,158,16],[159,29,161,29],[159,30,161,30],[159,31,161,31],[160,11,160,14],[153,29,156,29],[153,30,156,30],[153,31,156,31],[154,11,154,14],[155,11,155,14],[156,11,156,14],[153,23,156,23],[153,24,156,24],[153,25,156,25],[153,26,156,26],[153,27,156,27],[153,28,156,28],[153,17,156,17],[153,18,156,18],[153,19,156,19],[153,20,156,20],[153,21,156,21],[153,22,156,22],[147,11,147,14],[147,16,150,16],[151,29,152,29],[151,30,152,30],[151,31,152,31],[152,11,152,14],[153,1,156,2],[153,3,156,4],[153,5,156,6],[153,7,156,10],[153,11,153,14],[153,16,156,16],[151,23,152,23],[151,24,152,24],[151,25,152,25],[151,26,152,26],[151,27,152,27],[151,28,152,28],[151,17,152,17],[151,18,152,18],[151,19,152,19],[151,20,152,20],[151,21,152,21],[151,22,152,22],[147,1,152,2],[147,3,152,4],[147,5,150,6],[147,7,150,10],[151,5,152,6],[151,7,152,10],[151,11,151,14],[151,16,152,16],[145,11,145,14],[146,11,146,14],[142,24,146,24],[142,25,146,25],[142,26,146,26],[142,27,146,27],[142,28,146,28],[142,29,146,29],[142,18,146,18],[142,19,146,19],[142,20,146,20],[142,21,146,21],[142,22,146,22],[142,23,146,23],[147,29,150,29],[147,30,150,30],[147,31,150,31],[148,11,148,14],[149,11,149,14],[150,11,150,14],[147,23,150,23],[147,24,150,24],[147,25,150,25],[147,26,150,26],[147,27,150,27],[147,28,150,28],[147,17,150,17],[147,18,150,18],[147,19,150,19],[147,20,150,20],[147,21,150,21],[147,22,150,22],[137,19,138,19],[137,20,138,20],[137,21,138,21],[137,22,138,22],[137,11,137,14],[137,16,138,16],[139,30,140,30],[139,31,140,31],[140,11,140,14],[141,11,141,14],[142,3,146,4],[142,5,146,6],[142,7,146,10],[142,11,142,14],[142,16,146,16],[142,17,146,17],[139,24,140,24],[139,25,140,25],[139,26,140,26],[139,27,140,27],[139,28,140,28],[139,29,140,29],[139,18,140,18],[139,19,140,19],[139,20,140,20],[139,21,140,21],[139,22,140,22],[139,23,140,23],[142,30,146,30],[142,31,146,31],[143,11,143,14],[144,11,144,14],[137,29,138,29],[137,30,138,30],[137,31,138,31],[138,11,138,14],[134,1,146,2],[134,3,136,4],[134,5,136,6],[134,7,136,10],[134,11,134,14],[134,16,136,16],[134,29,136,29],[134,30,136,30],[134,31,136,31],[135,11,135,14],[136,11,136,14],[137,3,138,4],[137,5,138,6],[137,7,138,10],[139,3,141,4],[139,5,141,6],[139,7,141,10],[139,11,139,14],[139,16,140,16],[139,17,140,17],[137,23,138,23],[137,24,138,24],[137,25,138,25],[137,26,138,26],[137,27,138,27],[137,28,138,28],[137,17,138,17],[137,18,138,18],[132,11,132,14],[133,11,133,14],[129,24,133,24],[129,25,133,25],[129,26,133,26],[129,27,133,27],[129,28,133,28],[129,29,133,29],[129,18,133,18],[129,19,133,19],[129,20,133,20],[129,21,133,21],[129,22,133,22],[129,23,133,23],[134,23,136,23],[134,24,136,24],[134,25,136,25],[134,26,136,26],[134,27,136,27],[134,28,136,28],[134,17,136,17],[134,18,136,18],[134,19,136,19],[134,20,136,20],[134,21,136,21],[134,22,136,22],[126,30,127,30],[126,31,127,31],[127,11,127,14],[128,11,128,14],[129,3,133,4],[129,5,133,6],[129,7,133,10],[129,11,129,14],[129,16,133,16],[129,17,133,17],[126,24,127,24],[126,25,127,25],[126,26,127,26],[126,27,127,27],[126,28,127,28],[126,29,127,29],[126,18,127,18],[126,19,127,19],[126,20,127,20],[126,21,127,21],[126,22,127,22],[126,23,127,23],[126,3,128,4],[126,5,128,6],[126,7,128,10],[126,11,126,14],[126,16,127,16],[126,17,127,17],[129,30,133,30],[129,31,133,31],[130,11,130,14],[131,11,131,14],[124,28,125,28],[124,17,125,17],[124,18,125,18],[124,19,125,19],[124,20,125,20],[124,21,125,21],[124,22,125,22],[124,16,125,16],[121,23,123,23],[121,24,123,24],[121,25,123,25],[121,26,123,26],[121,27,123,27],[121,28,123,28],[121,17,123,17],[121,18,123,18],[121,19,123,19],[121,20,123,20],[121,21,123,21],[121,22,123,22],[124,29,125,29],[124,30,125,30],[124,31,125,31],[125,11,125,14],[118,30,120,30],[118,31,120,31],[119,11,119,14],[120,11,120,14],[121,1,133,2],[121,3,123,4],[121,5,123,6],[121,7,123,10],[121,11,121,14],[121,16,123,16],[118,24,120,24],[118,25,120,25],[118,26,120,26],[118,27,120,27],[118,28,120,28],[118,29,120,29],[118,18,120,18],[118,19,120,19],[118,20,120,20],[118,21,120,21],[118,22,120,22],[118,23,120,23],[116,1,120,2],[121,29,123,29],[121,30,123,30],[121,31,123,31],[122,11,122,14],[123,11,123,14],[124,3,125,4],[124,5,125,6],[124,7,125,10],[124,11,124,14],[118,3,120,4],[118,5,120,6],[118,7,120,10],[118,11,118,14],[118,16,120,16],[118,17,120,17],[116,23,117,23],[116,24,117,24],[116,25,117,25],[116,26,117,26],[116,27,117,27],[116,28,117,28],[116,17,117,17],[116,18,117,18],[116,19,117,19],[116,20,117,20],[116,21,117,21],[116,22,117,22],[116,3,117,4],[116,5,117,6],[116,7,117,10],[116,11,116,14],[116,16,117,16],[124,23,125,23],[124,24,125,24],[124,25,125,25],[124,26,125,26],[124,27,125,27],[114,11,114,14],[115,11,115,14],[113,22,115,22],[113,23,115,23],[113,24,115,24],[113,25,115,25],[113,26,115,26],[113,27,115,27],[113,16,115,16],[113,17,115,17],[113,18,115,18],[113,19,115,19],[113,20,115,20],[113,21,115,21],[116,29,117,29],[116,30,117,30],[116,31,117,31],[117,11,117,14],[110,29,112,29],[110,30,112,30],[110,31,112,31],[111,11,111,14],[112,11,112,14],[113,1,115,2],[113,3,115,4],[113,5,115,6],[113,7,115,10],[113,11,113,14],[110,23,112,23],[110,24,112,24],[110,25,112,25],[110,26,112,26],[110,27,112,27],[110,28,112,28],[110,17,112,17],[110,18,112,18],[110,19,112,19],[110,20,112,20],[110,21,112,21],[110,22,112,22],[110,1,112,2],[110,3,112,4],[110,5,112,6],[110,7,112,10],[110,11,110,14],[110,16,112,16],[113,28,115,28],[113,29,115,29],[113,30,115,30],[113,31,115,31],[106,30,107,30],[106,31,107,31],[107,11,107,14],[108,3,109,4],[108,5,109,6],[108,7,109,10],[108,11,108,14],[109,11,109,14],[106,22,107,22],[106,23,107,23],[106,24,107,24],[106,25,107,25],[106,26,107,26],[106,27,107,27],[106,16,107,16],[106,17,107,17],[106,18,107,18],[106,19,107,19],[106,20,107,20],[106,21,107,21],[106,1,109,2],[106,3,107,4],[106,5,107,6],[106,7,107,10],[106,11,106,14],[102,24,105,24],[102,25,105,25],[102,26,105,26],[102,27,105,27],[102,28,105,28],[102,29,105,29],[102,18,105,18],[102,19,105,19],[102,20,105,20],[102,21,105,21],[102,22,105,22],[102,23,105,23],[100,1,105,2],[106,28,107,28],[106,29,107,29],[100,29,101,29],[100,30,101,30],[100,31,101,31],[101,11,101,14],[102,3,105,4],[102,5,105,6],[102,7,105,10],[102,11,102,14],[102,16,105,16],[102,17,105,17],[100,23,101,23],[100,24,101,24],[100,25,101,25],[100,26,101,26],[100,27,101,27],[100,28,101,28],[100,17,101,17],[100,18,101,18],[100,19,101,19],[100,20,101,20],[100,21,101,21],[100,22,101,22],[100,3,101,4],[100,5,101,6],[100,7,101,10],[100,11,100,14],[100,16,101,16],[102,30,105,30],[102,31,105,31],[103,11,103,14],[104,11,104,14],[105,11,105,14],[79,16,84,16],[96,1,99,2],[96,3,99,4],[96,5,99,6],[96,7,99,10],[96,11,96,14],[97,11,97,14],[98,11,98,14],[99,11,99,14],[93,28,94,28],[93,29,94,29],[93,30,94,30],[93,31,94,31],[94,11,94,14],[95,11,95,14],[93,22,94,22],[93,23,94,23],[93,24,94,24],[93,25,94,25],[93,26,94,26],[93,27,94,27],[93,16,94,16],[93,17,94,17],[93,18,94,18],[93,19,94,19],[93,20,94,20],[93,21,94,21],[91,1,95,2],[91,3,92,4],[91,5,92,6],[91,7,92,10],[91,11,91,14],[93,3,95,4],[93,5,95,6],[93,7,95,10],[93,11,93,14],[85,30,90,30],[85,31,90,31],[86,11,86,14],[87,11,87,14],[88,11,88,14],[89,11,89,14],[90,11,90,14],[85,24,90,24],[85,25,90,25],[85,26,90,26],[85,27,90,27],[85,28,90,28],[85,29,90,29],[85,18,90,18],[85,19,90,19],[85,20,90,20],[85,21,90,21],[85,22,90,22],[85,23,90,23],[85,3,90,4],[85,5,90,6],[85,7,90,10],[85,11,85,14],[85,16,90,16],[85,17,90,17],[92,11,92,14],[77,22,78,22],[77,23,78,23],[77,24,78,24],[77,25,78,25],[77,26,78,26],[77,27,78,27],[77,16,78,16],[77,17,78,17],[77,18,78,18],[77,19,78,19],[77,20,78,20],[77,21,78,21],[79,29,84,29],[79,30,84,30],[79,31,84,31],[80,11,80,14],[81,11,81,14],[82,11,82,14],[83,11,83,14],[84,11,84,14],[79,23,84,23],[79,24,84,24],[79,25,84,25],[79,26,84,26],[79,27,84,27],[79,28,84,28],[79,17,84,17],[79,18,84,18],[79,19,84,19],[79,20,84,20],[79,21,84,21],[79,22,84,22],[77,1,90,2],[77,3,78,4],[77,5,78,6],[77,7,78,10],[77,11,77,14],[73,27,74,27],[73,28,74,28],[73,29,74,29],[73,30,74,30],[73,31,74,31],[74,11,74,14],[73,21,74,21],[73,22,74,22],[73,23,74,23],[73,24,74,24],[73,25,74,25],[73,26,74,26],[73,11,73,14],[73,16,74,16],[73,17,74,17],[73,18,74,18],[73,19,74,19],[73,20,74,20],[77,28,78,28],[77,29,78,29],[77,30,78,30],[77,31,78,31],[78,11,78,14],[79,3,84,4],[79,5,84,6],[79,7,84,10],[79,11,79,14],[71,1,76,2],[71,3,74,4],[71,5,72,6],[71,7,72,10],[71,11,71,14],[72,11,72,14],[73,5,74,6],[73,7,74,10],[69,25,70,25],[69,26,70,26],[69,27,70,27],[69,28,70,28],[69,29,70,29],[69,30,70,30],[69,19,70,19],[69,20,70,20],[69,21,70,21],[69,22,70,22],[69,23,70,23],[69,24,70,24],[67,1,70,2],[67,3,70,4],[75,3,76,4],[75,5,76,6],[75,7,76,10],[75,11,75,14],[76,11,76,14],[67,29,68,29],[67,30,68,30],[67,31,68,31],[68,11,68,14],[69,5,70,6],[69,7,70,10],[69,11,69,14],[69,16,70,16],[69,17,70,17],[69,18,70,18],[67,23,68,23],[67,24,68,24],[67,25,68,25],[67,26,68,26],[67,27,68,27],[67,28,68,28],[67,17,68,17],[67,18,68,18],[67,19,68,19],[67,20,68,20],[67,21,68,21],[67,22,68,22],[67,5,68,6],[67,7,68,10],[67,11,67,14],[67,16,68,16],[69,31,70,31],[70,11,70,14],[65,31,66,31],[66,11,66,14],[65,21,66,21],[65,22,66,22],[65,23,66,23],[65,24,66,24],[65,25,66,25],[65,26,66,26],[63,31,64,31],[64,11,64,14],[65,5,66,6],[65,7,66,10],[65,11,65,14],[65,16,66,16],[65,17,66,17],[65,18,66,18],[65,19,66,19],[65,20,66,20],[63,25,64,25],[63,26,64,26],[63,27,64,27],[63,28,64,28],[63,29,64,29],[63,30,64,30],[63,19,64,19],[63,20,64,20],[63,21,64,21],[63,22,64,22],[63,5,64,6],[63,7,64,10],[63,11,63,14],[62,1,66,2],[62,3,62,4],[62,5,62,6],[62,7,62,10],[62,11,62,14],[63,3,66,4],[58,25,61,25],[58,26,61,26],[58,27,61,27],[58,28,61,28],[58,29,61,29],[58,30,61,30],[58,19,61,19],[58,20,61,20],[58,21,61,21],[58,22,61,22],[58,23,61,23],[58,24,61,24],[53,1,61,2],[65,27,66,27],[65,28,66,28],[65,29,66,29],[58,16,61,16],[58,17,61,17],[58,18,61,18],[65,30,66,30],[55,23,57,23],[63,23,64,23],[63,24,64,24],[63,16,64,16],[63,17,64,17],[63,18,64,18],[53,31,54,31],[54,11,54,14],[55,3,61,4],[55,5,57,6],[55,7,57,10],[55,11,55,14],[55,16,57,16],[55,17,57,17],[53,23,54,23],[53,24,54,24],[53,25,54,25],[53,26,54,26],[53,27,54,27],[53,28,54,28],[53,17,54,17],[53,18,54,18],[53,19,54,19],[53,20,54,20],[58,31,61,31],[59,11,59,14],[60,11,60,14],[61,11,61,14],[53,3,54,4],[53,5,54,6],[53,7,54,10],[53,11,53,14],[53,16,54,16],[55,30,57,30],[55,31,57,31],[56,11,56,14],[57,11,57,14],[58,5,61,6],[58,7,61,10],[58,11,58,14],[48,7,52,10],[48,11,48,14],[48,16,52,16],[48,17,52,17],[48,18,52,18],[48,19,52,19],[48,31,52,31],[44,5,52,6],[44,7,47,10],[55,24,57,24],[55,25,57,25],[55,26,57,26],[55,27,57,27],[55,28,57,28],[55,29,57,29],[55,18,57,18],[55,19,57,19],[55,20,57,20],[55,21,57,21],[55,22,57,22],[44,25,47,25],[44,26,47,26],[44,27,47,27],[44,28,47,28],[44,29,47,29],[44,30,47,30],[44,19,47,19],[44,20,47,20],[44,21,47,21],[44,22,47,22],[53,29,54,29],[53,30,54,30],[41,22,43,22],[41,23,43,23],[48,26,52,26],[48,27,52,27],[48,28,52,28],[48,29,52,29],[48,30,52,30],[48,20,52,20],[48,21,52,21],[48,22,52,22],[48,23,52,23],[48,24,52,24],[48,25,52,25],[41,20,43,20],[41,21,43,21],[53,21,54,21],[53,22,54,22],[44,31,47,31],[45,11,45,14],[46,11,46,14],[47,11,47,14],[39,25,40,25],[39,26,40,26],[39,27,40,27],[39,28,40,28],[39,17,40,17],[39,18,40,18],[39,19,40,19],[39,20,40,20],[39,21,40,21],[39,22,40,22],[44,23,47,23],[44,24,47,24],[41,30,43,30],[41,31,43,31],[42,11,42,14],[43,11,43,14],[44,11,44,14],[44,16,47,16],[44,17,47,17],[44,18,47,18],[41,24,43,24],[41,25,43,25],[41,26,43,26],[41,27,43,27],[41,28,43,28],[41,29,43,29],[41,18,43,18],[41,19,43,19],[39,1,52,2],[39,3,40,4],[39,5,40,6],[39,7,40,10],[39,11,39,14],[39,16,40,16],[49,11,49,14],[50,11,50,14],[51,11,51,14],[52,11,52,14],[36,1,38,2],[36,3,38,4],[36,5,38,6],[36,7,38,10],[36,11,38,15],[36,16,36,31],[37,16,37,19],[37,20,37,23],[37,24,37,27],[37,28,37,31],[39,29,40,29],[39,30,40,30],[39,31,40,31],[40,11,40,14],[41,3,52,4],[41,5,43,6],[41,7,43,10],[41,11,41,14],[41,16,43,16],[41,17,43,17],[39,23,40,23],[39,24,40,24],[32,1,32,2],[32,3,32,4]],"merged_total":1067,"flags":["merged_cut"]}
[]
[null,"2.1-1. Natural Gas Production and Procurement Plan"]
[]
[null,"❚Provide information about the processes related to the upstream emissions from natural gas used as a raw material and fuel for hydrogen production to estimate the associated emissions."]
[null,"❚Input of detailed factors at each stage of the upstream process related to natural gas production is necess"]
[null,"   (LNG process stages: 1. Recovery 2. Processing 3. Pipeline T&D 4. Liquefaction 5. Shipment 6. Domestic storage, regasification, distribution)"]
[null,"   (PNG process stages: 1. Recovery 2. Processing 3. Pipeline T&D)"]
[null,"❚If information on a particular process is lacking, please provide an explanation in the 'Remarks' section (e.g., If the extraction and refinement processes are integrated: Enter the information about the mixed process under the extraction process, leave the refinement process blank, and provide an explanation in the 'Remarks' section)."]
[]
[null,"Process Input","Major Category","Sub-category","Code of origin","Input(output) name","Unit","Amount","Natural Gas LHV[MJ/kg]","1-1. Recovery -\n Process Fuel Usage[MJ/MJ]*","1-2. Recovery -\n NG flaring [J/MJ]**","1-3. Recovery -\n CH4: Non combustion [g/MJ]***","2-1. Processing -\n Process Fuel Usage[MJ/MJ]*","2-2. Processing -\n NG flaring [J/MJ]**","2-3. Processing -\n CO2: Non combustion [g/MJ]****","2-4. Processing -\n CH4: Non combustion [g/MJ]***","3-1. Pipeleine T&D -\n distance[km]",null,"3-2. Pipeline T&D -\n Energy intensity [J/t-km]*****",null,"3-3. Pipeline T&D -\nCH4 leakage [g/MJ-km]******",null,"4-1. Liquefaction -\n  Process Fuel Usage[MJ/MJ]*",null,"4-2. Liquefaction -\n NG flaring [J/MJ]**",null,"4-3. Liquefaction -\n CH4: Non-combustion [g/MJ]***",null,"5-1. Shipment - distance[km]",null,"5-2. Shipment -\n Energy intensity(abroad->Korea) [J/t-km]*****",null,"5-3. Shipment - Energy intensity(Korea->abroad)\n [J/t-km]*****",null,"6. Domestic Storage, Regasification, Distribution - Process Fuel Usage[MJ/MJ]*",null,"Remark"]
[]
[]
[]
[]
[]
[null,"* Process Fuel Usage: The total energy amount (MJ) based on the LHV of the process fuel used per unit of product energy (MJ) for the relevant process (e.g., Enter the usage each fuel: 0.1 MJ electricity + 0.2 MJ natural gas)"]
[null,"** NG flaring: The energy amount (J) of NG flared per unit of product energy (MJ) in the relevant process."]
[null,"*** CH4: Non-combustion: The mass (g) of NG released into the atmosphere through leakage or venting per unit of product energy (MJ) in the relevant process. Enter the net leak amount remaining after flaring."]
[null,"**** CO2: Non-combustion: The amount of non-combustion CO2 emissions (g) per unit of product energy (MJ) emitted during the natural gas refinement process (e.g., removal of CO2 included in raw NG)"]
[null,"***** Transport Energy Intensity: The energy usage (J) consumed to transport a unit mass (ton) of natural gas product over a unit distance (km)"]
[null,"****** Pipeline CH4 leakage: The leakage amount (g) that occurs when transporting a unit energy amount (MJ) of natural gas product over a unit distance (km) through the pipeline."]
[]
[]
[null,"2.1-2. Detailed emission reporting sheet for each process on natural gas production and procurement "]
[]
[null,"❚Provide process-specific emissions information to calculate upstream emissions of natural gas used as feedstock and fuel for hydrogen production"]
[null,"❚Calculate process-specific emissions and fill total sum in on table 2-1.1"]
[null,"❚If it is planned to connect to a specific gas field, at least the gas field type must be filled in"]
[null,"❚Indicate which standard(ex. ISO, ASTM, etc.) the measurement complies with and sumbit verification* per parameter when using measurement data"]
[null,"❚The following process classification is an example and may be modified. Only verifiable measurement-based figures are accepted"]
[]
[null,"Gas Field Type (Indicate as Applicable)"]
[null,"Type of Reservoir",null,"Gas Association Type",null,"Location of development"]
[null,"Conventional / Unconventional",null,"Associated / Non-associated",null,"Onshore / Offshore"]
[]
[null,"Emissions input sheet per process"]
[null,"Subject of reporting",null,"Conditions for measurement",null,"Measurement methods",null,"Emission calculation formoula**",null,null,null,"Information for calculation",{"$nulls":4},"Emissions by process (kg/MJ)"]
[{"$nulls":16},"Recovery",null,null,null,"Processing",null,null,null,"Pipmeline T&D",null,null,null,"Liquefaction"]
[{"$nulls":16},"CO2","CH4","N2O","others","CO2","CH4","N2O","others","CO2","CH4","N2O","other","CO2","CH4","N2O","others"]
[null,"Natural gas pneumatic device",null,"If a continuous flowmeter \nis available",null,"Use continuous flowmeter",null,"(예시)",null,null,null,"- Flow rate measured by a continuous flowmeter",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Mole fraction of CO2 and CH4 in produced or processed gas",null,null,null,"Test standards or\n sources related to data"]
[null,null,null,"Select if continuous flowmeter\n is not available",null,"Use temporary flowmeter\n(calibrated bagging,\n high volume sampler, etc.)",{"$nulls":5},"- Used flow measurement method used and measured flow rate",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- The period during which the flow was measured",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Concentration of CO2 and CH4 in produced or processed gas",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":5},"Use emission factors",null,"○ A calculation formula for continuous bleed pneumatic devices",null,null,null,"- Number of devices by type",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Concentration of CO2 and CH4 in produced or processed gas",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Average operating time of devices obtained from engineering estimates",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Emission factor values used in the calculation",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":7},"○ A calculation formula for intermittent bleed pneumatic devices",null,null,null,"- Concentration of CO2 and CH4 in gas supplied to the divice",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- The total number of devices with malfunctions detected during device inspection",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- The total time the device was in operation during the year and the time it malfunctioned",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- The total number of devices for which emissions were calculated using the method",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Emission factor values used in the calculation",null,null,null,"Test standards or\n sources related to data"]
[null,"Natural gas driven\n pneumatic pump",null,"If a continuous flowmeter\n is available",null,"Use continuous flowmeter",{"$nulls":5},"- Flow rate measured by a continuous flowmeter",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Mole fraction of CO2 and CH4 in produced or processed gas",null,null,null,"Test standards or\n sources related to data"]
[null,null,null,"Select if continuous flowmeter\nis not available",null,"Use temporary flowmeter\n(calibrated bagging, \nhigh volume sampler, etc.)",{"$nulls":5},"- Used flow measurement method used and measured flow rate",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- The period during which the flow was measured",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Mole fraction of CO2 and CH4 in produced gas",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":5},"Use emission factors",{"$nulls":5},"- The total number of devices",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Concentration of CO2 and CH4 in produced or processed gas",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Average operating time of the device obtained from engineering estimates",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Emission factor values used in the calculation",null,null,null,"Test standards or\n sources related to data"]
[null,"Acid gas removal unit",null,"If a CEMS is available",null,"Use CEMS",{"$nulls":5},"- Flow rate and concentration of CO2 measured by a CEMS",null,null,null,"Test standards or\n sources related to data"]
[null,null,null,"Select if CEMS is not available",null,"Use vent meter that can measure the concentration of the gas",{"$nulls":5},"- Annual average CO2 and CH4 volume fraction in vent gas ",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Annual emissions volume of vent gas",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":5},"Use continuous flowmeter",{"$nulls":5},"- Emissions volume from the inlet/outlet gas",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Average CO2 and CH4 volume fraction of inlet inlet/outlet gas ",null,null,null,"Test standards or\n sources related to data"]
[null,"Nitrogen removal unit",null,"Select ",null,"Use vent meter that can measure the concentration of the gas",{"$nulls":5},"- Annual average CO2 and CH4 volume fraction in vent gas ",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Annual emissions volume of vent gas",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":5},"Use continuous flowmeter",{"$nulls":5},"- Emissions volume from the inlet/outlet gas",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Average CO2 and CH4 volume fraction of vent gas",null,null,null,"Test standards or\n sources related to data"]
[null,"Dehydrator",null,"Use according to the type of dehydrator",null,"Use emission factors",null,"○ A calculation formula for glycol dehydrators",null,null,null,"- Total number of dehydrators using same method",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Emission factor values used in the calculation",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":5},"Measurement of pressure",null,"○ A calculation formula for desiccant dehydrators",null,null,null,"- Number of decompressions of dehydrators per year",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Gas pressure",null,null,null,"Test standards or\n sources related to data"]
[null,null,null,"If the dehydrator is routed to\na regenerator firebox/fire tubes or other non-flare combustion devices",null,"Use continuous flowmeter or CEMS, and continuous composition analyzer",{"$nulls":5},"- Used flow measurement method used and measured flow rate",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Gas composition",null,null,null,"Test standards or\n sources related to data"]
[null,"Well venting for liquid unloading",null,"If a flowmeter is available",null,"Use flowmeter",{"$nulls":5},"- Average flow rate",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Duration of venting",null,null,null,"Test standards or\n sources related to data"]
[null,null,null,"If the flowmeter is not available\n and work without a flinger lift",null,"Measurement of\ntemperature and pressure",{"$nulls":5},"- Number of extractions performed in the well during the monitoring period",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Well diameter",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Well depth ",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Well pressure",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Average flow rate in the well",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Time the well was exposed to the atmosphere during operation",null,null,null,"Test standards or\n sources related to data"]
[null,null,null,"If the flowmeter is not available\n and work with a flinger lift",null,"Measurement of\ntemperature and pressure",{"$nulls":5},"- Number of extractions performed in the well during the monitoring period",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Well diameter",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Well depth ",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Well pressure",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Average flow rate in the well",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Duration the well was exposed to the atmosphere during operation",null,null,null,"Test standards or\n sources related to data"]
[null,"Well venting during\n well completions and workovers with hydraulic fracturing",null,"If a flowmeter is available",null,"Flowmeter",{"$nulls":5},"- Measured gas flowback rate using a flowmeter",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- FRMs and FRMi values used in the calculation",null,null,null,"Test standards or\n sources related to data"]
[null,null,null,"If the flowmeter is not available",null,"Measurement of\n temperature and pressure",{"$nulls":5},"- well choke valve upstream and downstream pressure",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- well choke valve upstream temperature",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- FRMs and FRMi values used in the calculation",null,null,null,"Test standards or\n sources related to data"]
[null,"Well venting during\n well completions and workovers without hydraulic fracturing",null,"No conditions for using",null,"Use emission factors",{"$nulls":5},"- Annual natural gas emissions from oil wells",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Daily gas production rate from oil wells",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Duration when gas is directly released into the atmosphere",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Emission factor values used in the calculation",null,null,null,"Test standards or\n sources related to data"]
[null,"Blowdown vent stacks",null,"If a flowmeter is available",null,"Use continuous flowmeter",{"$nulls":5},"- Flow rate measured by a continuous flowmeter",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Mole fraction of CO2 and CH4 in vent gas",null,null,null,"Test standards or\n sources related to data"]
[null,null,null,"If a flowmeter is not available",null,"Measurement of\ntemperature and pressure",{"$nulls":5},"- Number of blowdowns",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Volume of blowdown vent stack",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Measured temperature and pressure",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Compression factor used in the calculation",null,null,null,"Test standards or\n sources related to data"]
[null,"Hydrocarbon liquids\nand produced water\nstorage tank",null,"If the average daily throughput of the tank is 10 barrels or more",null,"Use temporary flowmeter\n(high volume sampler)",{"$nulls":5},"- Annual gas emissions from tanks",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- CO2 and CH4 volume/mass fraction of hydrocarbon liquid-derived gases",null,null,null,"Test standards or\n sources related to data"]
[null,null,null,"No conditions for using",null,"Use emission factors",{"$nulls":5},"- Total number of tanks using same calculation method",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Emission factor values used in the calculation",null,null,null,"Test standards or\n sources related to data"]
[null,"Condensate storage tank",null,"If a leak is detected during monitoring",null,"Available method among\ntemporary flowmeter\n(calibrated bagging, \nhigh volume sampler, etc.),\n Optical gas imaging instrument, Acoustic leak detection device",{"$nulls":5},"- Used flow measurement method used and measured flow rate",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- The period during which the flow was measured",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Mole or mass fraction of CO2 and CH4 in produced or processed gas",null,null,null,"Test standards or\n sources related to data"]
[null,"Well testing",null,"No conditions for using",null,"Use flowmeter",{"$nulls":5},"- GOR value used for calculation",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Average annual daily production of the gas field under test",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Number of days the well was tested",null,null,null,"Test standards or\n sources related to data"]
[null,"Associated Gas",null,"If a continuous flowmeter is\n available",null,"Use continuous flowmeter",{"$nulls":5},"- Measured flow rate value",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Mole fraction of CO2 and CH4 in the associated gas",null,null,null,"Test standards or\n sources related to data"]
[null,null,null,"If a continuous flowmeter is\nnot available",null,"-",{"$nulls":5},"- GOR value used for calculation",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Amount of crude oil produced during the emission of associated gas",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- The amount of associated gas used to supply power to engines, combustion equipment, etc.",null,null,null,"Test standards or\n sources related to data"]
[null,"Centrifugal compressor",null,"In case of measurement",null,"Available method among\ntemporary flowmeter\n(calibrated bagging, \nhigh volume sampler, etc.),\n Optical gas imaging instrument, Acoustic leak detection device",{"$nulls":5},"- Volume emissions from the compressor",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Duration of emissions",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Volumetric emissions of CO2 and CH4 in vent gas",null,null,null,"Test standards or\n sources related to data"]
[null,null,null,"In case of continuous monitoring",null,"Use flowmeter\nand composition analyzer",{"$nulls":5},"- Volume emissions from the compressor",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Mole emissions of CO2 and CH4 in vent gas",null,null,null,"Test standards or\n sources related to data"]
[null,null,null,"If measurement is impossible",null,"Use emission factors",{"$nulls":5},"-  Average volume emissions from the compressor",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Total number of compressors measured",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Emission factor values used in the calculation",null,null,null,"Test standards or\n sources related to data"]
[null,null,null,"In case of wet seal oill degassing",null,"Use emission factors",{"$nulls":5},"- Total number of compressors using this method",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Total time the compressors were running",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Volumetric emissions of CO2 and CH4 ",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Mole fraction of CO2 and CH4",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Emission factor values used in the calculation",null,null,null,"Test standards or\n sources related to data"]
[null,"Reciprocating compressor",null,"In case of measurement",null,"Available method among\ntemporary flowmeter\n(calibrated bagging, \nhigh volume sampler, etc.),\n Optical gas imaging instrument, Acoustic leak detection device",{"$nulls":5},"- Volume emissions from the compressor",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Duration of emissions",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Volumetric emissions of CO2 and CH4 in vent gas",null,null,null,"Test standards or\n sources related to data"]
[null,null,null,"In case of continuous monitoring",null,"Use flowmeter\nand composition analyzer",{"$nulls":5},"- Volume emissions from the compressor",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Mole emissions of CO2 and CH4 in vent gas",null,null,null,"Test standards or\n sources related to data"]
[null,null,null,"If measurement is impossible",null,"Use emission factors",{"$nulls":5},"- Average volume emissions from the compressor",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Total number of compressors measured",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Emission factor values used in the calculation",null,null,null,"Test standards or\n sources related to data"]
[null,null,null,"In case of rod packing",null,"Use emission factors",{"$nulls":5},"- Total number of compressors using this calculation method",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Volumetric emissions of CO2 and CH4",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Total time the compressors were running",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Emission factor values used in the calculation",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Mole fraction of CO2 and CH4",null,null,null,"Test standards or\n sources related to data"]
[null,"Equipment leaks",null,"Select using emission factors or \nthe leakage measurement",null,"Use emission factors",{"$nulls":5},"- Number of each facility using this method",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Duration when the equipment leake",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- CO2 and CH4 concentration used in the calculation",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Emission factor used in the calculation",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":5}," Measurement of\nleakage point",{"$nulls":5},"- Used measurement method and the measured leakage flow rate",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Duration the leakage continued",null,null,null,"Test standards or\n sources related to data"]
[null,"EOR injection pump",null,"No conditions for using",null,"-",{"$nulls":5},"- Number of blowdowns of EOR pump",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- System chamber volume of EOR injection pump",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Density of EOR injection gas",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Mass fraction of CO2 in injection gas",null,null,null,"Test standards or\n sources related to data"]
[null,"EOR hydrocarbon liquids",null,"No conditions for using",null,"-",{"$nulls":5},"- The amount of CO2 remaining in the hydrocarbon liquid in the tank",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- The total amount of hydrocarbon liquid produced by EOR during the year",null,null,null,"Test standards or\n sources related to data"]
[null,"Other large release events",null,"No conditions for using",null,"-",{"$nulls":5},"- Duration of the emission event",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Measured emission rate",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Measured composition of CO2 and CH4 in the emission gas",null,null,null,"Test standards or\n sources related to data"]
[null,"Drilling Mud Degassing",null,"If measuring composition\nusing a gastrap at all times",null,"Use a gastrap",{"$nulls":5},"- The rate of gas emissions from the drilling mud degassing",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- The average concentration of the vent gas measured by a gastrap",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Mole fraction of each component in drilling mud",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Duratin of the drilling mud circulation was sustained",null,null,null,"Test standards or\n sources related to data"]
[null,null,null,"If measuring composition\n using a gastrap only at part of time",null,"Use a gastrap,\nmeasurement of composition",{"$nulls":5},"- The rate of gas emissions from the drilling mud degassing",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- The average concentration of the vent gas measured by a gastrap",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Mole fraction of each component in drilling mud",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Type of drilling mud used (aqueous, oil-based, or synthetic)",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Number of days drilling continued",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Duratin of the drilling mud circulation was sustained'",null,null,null,"Test standards or\n sources related to data"]
[null,null,null,"Not using a gastrap",null,"Measurement of composition",{"$nulls":5},"- Type of drilling mud used (aqueous, oil-based, or synthetic)",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Number of days drilling continued",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Mole fraction of each component in drilling mud",null,null,null,"Test standards or\n sources related to data"]
[null,"Crankcase",null,"If the flow rate\n is measured",null,"Use temporary flowmeter\n(calibrated bagging,\nhigh volume sampler, etc.)",{"$nulls":5},"- Used measurement method and the measured flow rate",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- The concentration of components of feed into the reciprocating internal combustion engine",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- The total operating time of the reciprocating internal combustion engine",null,null,null,"Test standards or\n sources related to data"]
[null,null,null,"If the flow rate is not measured",null,"Use emission factors",{"$nulls":5},"- The total operating time of the reciprocating internal combustion engine",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Emission factor used in the calculation",null,null,null,"Test standards or\n sources related to data"]
[null,"Flare stack",null,"Calculate emissions by combining each item",null,"Measurement of\ncomposition and flow rate",{"$nulls":5},"- Destruction efficiency",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Combustion efficiency",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Period when the flare stack is turned off",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Volume fraction of each component",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Use the flow rate flowing into the flare stack from each device",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Mole fraction of each component",null,null,null,"Test standards or\n sources related to data"]
[null,"Combustion equipment***",null,"Select according to fuel specifications",null,"Use emission factors",null,"○ If the fuel meets the pipeline quality and has a minimum higher heating value of 950 or more Btu/ft3\n○ When the higher heating value of fuel is 950-1,100 Btu and the volume fraction of methane is 70% or more",null,null,null,"- The performance test method and the emission factor derived from it",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Information of equipment manufacturer such as manufacturer specifications and emission certification data",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":5},"Measurement of\ncomposition and flow rate",null,"○ If the fuel is not of pipeline quality or has a minimum higher heating value of less than 950 Btu/ft3.",null,null,null,"- Annual gas volume entering the combustion device (using measured or engineering estimates)",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Mole fraction of each component of the gas entering the combustion device",null,null,null,"Test standards or\n sources related to data"]
[{"$nulls":11},"- Combustion device type",null,null,null,"Test standards or\n sources related to data"]
[null,"* Indicate the page number where the key information is described in the verificaiton"]
[null,"** Enter the formula used in the calculation"]
[null,"*** Process fuel use: Emissions from the combustion of fuel supplied for the operation of each facility"]

{"sheet":"2.2. Feed Pre-treatment","index":9,"n_rows":42,"n_cols":15,"rows_kept":42,"cut":false,"hidden":false,"merged":[[11,14,11,15],[10,14,10,15],[16,14,16,15],[15,14,15,15],[14,14,14,15],[13,14,13,15],[12,14,12,15],[27,10,27,11],[26,5,27,6],[1,1,1,6],[3,1,3,15],[4,1,4,15],[6,1,6,6],[5,1,5,3],[5,4,5,15],[8,14,9,15],[23,14,23,15],[22,14,22,15],[21,14,21,15],[20,14,20,15],[19,14,19,15],[18,14,18,15],[17,14,17,15],[7,1,7,6],[8,1,9,2],[8,3,9,3],[8,4,9,4],[8,5,9,5],[8,6,9,6],[10,1,16,1],[17,1,23,1],[8,7,9,7],[8,8,9,8],[8,9,9,9],[26,13,27,15],[33,2,33,3],[8,12,9,12],[8,13,9,13],[8,10,9,10],[8,11,9,11],[32,2,32,3],[29,2,29,3],[31,2,31,3],[33,10,33,11],[28,2,28,3],[25,1,25,6],[26,1,27,1],[26,2,27,3],[26,4,27,4],[26,7,26,12],[33,13,33,15],[32,13,32,15],[31,13,31,15],[29,13,29,15],[32,10,32,11],[31,10,31,11],[29,10,29,11],[28,13,28,15],[30,2,30,3],[30,10,30,11],[30,13,30,15],[28,10,28,11],[28,5,28,6],[33,5,33,6],[32,5,32,6],[31,5,31,6],[30,5,30,6],[29,5,29,6]]}
[]
[null,"2.2. Unit process name : Feed Pre-treatment/Fired heater"]
[null,"❚Unit Process PFD"]
[null,"Unit Process PFD"]
[]
[null,"Process Description"]
[]
[null,"❚Continuous input(output) material and energy stream data",{"$nulls":9},"※For electricity, enter the kWh used per hour (kWh/hr)"]
[null,"  ",null,"Main Category","Sub-category","Origin","Input(output) name","Unit","Amount","Density\n(kg/Nm3)","LHV\n(MJ/kg)","Composition\n(mol%)","Calculation basis","Data source ","Remarks\n(For steam,\nTemp.(°C)/Press.(bar))"]
[]
[null,"Input","①","Raw material for hydrogen production","Natural gas\nImported natural gas","AUSTRALIA","NG\n[From outside the system boundary]","kg/hr",50000,null,null,null,"Self-calculation\nbased on\nspecification","PFD"]
[null,null,"②","Main Fuel for hydrogen production facilities","Natural gas\nDomestic city gas","KOREA, REPUBLIC OF","LNG\n[From outside the system boundary]","kg/hr",10000,null,null,null,"Self-calculation\nbased on\nspecification","PFD"]
[null,null,"③","Electricity","Electricity\nOther electricity","KOREA, REPUBLIC OF","Electricity\n[From 2.2-Out-8]","kWh",10000,null,null,null,"Self-calculation\nbased on\nspecification","PFD"]
[null,null,"④","Other input material","Common\nIndustrial water","KOREA, REPUBLIC OF","Process water\n[From outside the system boundary]","kg/hr",10000,null,null,null,"Self-calculation\nbased on\nspecification","PFD","  "]
[null,null,"⑤"]
[null,null,"⑥",{"$nulls":5},"  ",{"$nulls":4},"  ","  "]
[null,null,"⑦"]
[null,"Output","⑧","Intermediate product","Other raw materials","KOREA, REPUBLIC OF","Pre-treated material\n[To 2.4-In-1]","kg/hr",30000,null,null,null,"Simulation","PFD"]
[null,null,"⑨","Waste","Waste","KOREA, REPUBLIC OF","Flue gas\n[To outside the system boundary]","kg/hr",10000,null,null,null,"Simulation","Flow meter"]
[null,null,"⑩"]
[null,null,"⑪"]
[null,null,"⑫",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑬",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑭",null,null,null,"  ","  ","  ",{"$nulls":5},"  "]
[]
[null,"❚Discontinuous input(output) stream data"]
[null,"Input\n(Output)","Main Category",null,"Sub-category","Input(Output) name",null,"Detailed Information",{"$nulls":5},"Remarks"]
[{"$nulls":7},"Annual\ninput(output) ammount","(Bulk) density","Active Ingredients","Detailed composition\n(including solvent)",null,"CAS No."]
[null,"Input","Other input material",null,"Chemical substance","Raw water treatment-\nCitric Acid aqueous solution\n[From outside the system boundary]",null,"7200 kg/yr","-","Citric Acid","Citric Acid (50 %)\nWater (50 %)",null,"77-92-9\n7732-18-5"]
[null,"Input","Other input material",null,"Chemical substance","Boiler Condensate Treatment\n[From outside the system boundary]",null,"12.1865 m3/yr","1.03 kg/m3","Ethanolamine","Ethanolamine (85 %)\nDiethanolamine (15 %)",null,"141-43-5\n111-42-2"]
{"$rows_empty":9}
[{"$nulls":13},"  ","  "]
[{"$nulls":13},"  ","  "]
[{"$nulls":13},"  ","  "]

{"sheet":"2.3. Pre-reformer","index":10,"n_rows":28,"n_cols":15,"rows_kept":28,"cut":false,"hidden":false,"merged":[[19,14,19,15],[20,14,20,15],[21,14,21,15],[22,14,22,15],[23,14,23,15],[33,10,33,11],[33,13,33,15],[1,1,1,6],[3,1,3,15],[4,1,4,15],[26,7,26,12],[26,13,27,15],[5,1,5,3],[5,4,5,15],[7,1,7,6],[8,1,9,2],[8,3,9,3],[8,4,9,4],[8,5,9,5],[8,6,9,6],[8,7,9,7],[8,8,9,8],[10,1,16,1],[17,1,23,1],[28,2,28,3],[29,2,29,3],[25,1,25,6],[26,1,27,1],[26,2,27,3],[26,4,27,4],[26,5,27,6],[28,5,28,6],[29,5,29,6],[8,9,9,9],[8,10,9,10],[8,11,9,11],[8,12,9,12],[8,13,9,13],[27,10,27,11],[28,10,28,11],[28,13,28,15],[29,10,29,11],[29,13,29,15],[8,14,9,15],[10,14,10,15],[11,14,11,15],[12,14,12,15],[13,14,13,15],[14,14,14,15],[15,14,15,15],[16,14,16,15],[17,14,17,15],[18,14,18,15],[30,10,30,11],[30,13,30,15],[31,10,31,11],[31,13,31,15],[32,10,32,11],[32,13,32,15],[33,2,33,3],[32,2,32,3],[30,2,30,3],[31,2,31,3],[30,5,30,6],[31,5,31,6],[32,5,32,6],[33,5,33,6]]}
[]
[null,"2.3. Unit process name : Pre-reformer"]
[null,"❚Unit Process PFD"]
[null,"Unit Process PFD"]
[]
[null,"Process Description"]
[]
[null,"❚Continuous input(output) material and energy stream data",{"$nulls":9},"※For electricity, enter the kWh used per hour (kWh/hr)"]
[null,"  ",null,"Main Category","Sub-category","Origin","Input(output) name","Unit","Amount","Density\n(kg/Nm3)","LHV\n(MJ/kg)","Composition\n(mol%)","Calculation basis","Data source ","Remarks\n(For steam,\nTemp.(°C)/Press.(bar))"]
[]
[null,"Input","①","Intermediate product","Other raw materials","KOREA, REPUBLIC OF","Pre-treated material\n[From 2.3-Out-8]","kg/hr",30000,null,null,null,"Self-calculation\nbased on\nspecification","PFD"]
[null,null,"②","Main Fuel for hydrogen production facilities","Heat\n(Steam, based on ~~~)","KOREA, REPUBLIC OF","Steam\n[From 2.5-Out-9]","kg/hr",10,null,null,null,"Self-calculation\nbased on\nspecification","PFD"]
[null,null,"③","Electricity","Electricity\nOther electricity","KOREA, REPUBLIC OF","Electricity\n[From 2.2-Out-9]","kWh",10000,null,null,null,"Self-calculation\nbased on\nspecification","Power Meter"]
[null,null,"④",{"$nulls":11},"  "]
[null,null,"⑤"]
[null,null,"⑥",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑦"]
[null,"Output","⑧","Intermediate product","Other raw materials","KOREA, REPUBLIC OF","Pre-reformed material\n[To 2.5-In-1]","kg/hr",4900,null,null,null,"Self-calculation\nbased on\nspecification","PFD"]
[null,null,"⑨"]
[null,null,"⑩"]
[null,null,"⑪"]
[null,null,"⑫",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑬",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑭",null,null,null,"  ","  ","  ",{"$nulls":5},"  "]
[]
[null,"❚Discontinuous input(output) stream data"]
[null,"Input\n(Output)","Main Category",null,"Sub-category","Input(Output) name",null,"Detailed Information",{"$nulls":5},"Remarks"]
[{"$nulls":7},"Annual\ninput(output) ammount","(Bulk) density","Active Ingredients","Detailed composition\n(including solvent)",null,"CAS No."]

{"sheet":"2.4. Reformer(ATR, SMR, etc)","index":11,"n_rows":28,"n_cols":15,"rows_kept":28,"cut":false,"hidden":false,"merged":[[19,14,19,15],[20,14,20,15],[21,14,21,15],[22,14,22,15],[23,14,23,15],[14,14,14,15],[15,14,15,15],[16,14,16,15],[17,14,17,15],[18,14,18,15],[8,14,9,15],[10,14,10,15],[11,14,11,15],[12,14,12,15],[13,14,13,15],[32,10,32,11],[32,13,32,15],[33,5,33,6],[33,10,33,11],[33,13,33,15],[30,10,30,11],[30,13,30,15],[31,5,31,6],[31,10,31,11],[31,13,31,15],[27,10,27,11],[28,5,28,6],[28,10,28,11],[28,13,28,15],[29,5,29,6],[29,10,29,11],[29,13,29,15],[26,13,27,15],[26,5,27,6],[26,7,26,12],[1,1,1,6],[3,1,3,15],[4,1,4,15],[5,1,5,3],[5,4,5,15],[7,1,7,6],[8,1,9,2],[8,3,9,3],[8,4,9,4],[8,5,9,5],[8,6,9,6],[8,9,9,9],[8,10,9,10],[8,11,9,11],[8,12,9,12],[8,8,9,8],[8,13,9,13],[31,2,31,3],[33,2,33,3],[10,1,16,1],[17,1,23,1],[25,1,25,6],[26,1,27,1],[26,2,27,3],[26,4,27,4],[32,2,32,3],[29,2,29,3],[30,2,30,3],[28,2,28,3],[8,7,9,7],[30,5,30,6],[32,5,32,6]]}
[]
[null,"2.4. Unit process name : Reformer(ATR, SMR etc)",{"$nulls":5},"※Specify the applicable types"]
[null,"❚Unit Process PFD"]
[null,"Unit Process PFD"]
[]
[null,"Process Description"]
[]
[null,"❚Continuous input(output) material and energy stream data",{"$nulls":9},"※For electricity, enter the kWh used per hour (kWh/hr)"]
[null,"  ",null,"Main Category","Sub-category","Origin","Input(output) name","Unit","Amount","Density\n(kg/Nm3)","LHV\n(MJ/kg)","Composition\n(mol%)","Calculation basis","Data source ","Remarks\n(For steam,\nTemp.(°C)/Press.(bar))"]
[]
[null,"Input","①","Intermediate product","Other raw materials","KOREA, REPUBLIC OF","Pre-reformed material\n[From 2.4-Out-8]","kg/hr",4900,null,null,null,"Simulation","PFD"]
[null,null,"②","Electricity","Electricity\nOther electricity","KOREA, REPUBLIC OF","Electricity\n[From 2.2-Out-10]","kWh",10000,null,null,null,"Simulation","Power Meter"]
[null,null,"③","Other raw materials","Other raw materials","KOREA, REPUBLIC OF","Oxygen(O2)\n[From outside the system boundary]","kg/hr",10,null,null,null,"Simulation","PFD"]
[null,null,"④","Fuel for raw material production facility for hydrogen production","Heat\n(Steam, based on ~~~)","KOREA, REPUBLIC OF","Steam\n[From 2.5-Out-9]","kg/hr",10,null,null,null,"Simulation","PFD","  "]
[null,null,"⑤"]
[null,null,"⑥",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑦"]
[null,"Output","⑧","Intermediate product","Other raw materials","KOREA, REPUBLIC OF","Syngas\n[To 2.6-In-1]","kg/hr",4900,null,null,null,"Simulation","Mass Flow Meter"]
[null,null,"⑨","Other by products","Heat\n(Steam, based on ~~~)","KOREA, REPUBLIC OF","Steam\n[To 2.4-In-2][To 2.5-In-4]\n[To 2.6-In-2]","kg/hr",30,null,null,null,"Simulation","PFD"]
[null,null,"⑩"]
[null,null,"⑪"]
[null,null,"⑫",{"$nulls":11},"  "]
[null,null,"⑬",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑭",null,null,null,"  ","  ","  ",{"$nulls":5},"  "]
[]
[null,"❚Discontinuous input(output) stream data"]
[null,"Input\n(Output)","Main Category",null,"Sub-category","Input(Output) name",null,"Detailed Information",{"$nulls":5},"Remarks"]
[{"$nulls":7},"Annual\ninput(output) ammount","(Bulk) density","Active Ingredients","Detailed composition\n(including solvent)",null,"CAS No."]

{"sheet":"2.5. Water Gas Shift Reactor","index":12,"n_rows":28,"n_cols":15,"rows_kept":28,"cut":false,"hidden":false,"merged":[[19,14,19,15],[20,14,20,15],[21,14,21,15],[22,14,22,15],[23,14,23,15],[14,14,14,15],[15,14,15,15],[16,14,16,15],[17,14,17,15],[18,14,18,15],[8,14,9,15],[10,14,10,15],[11,14,11,15],[12,14,12,15],[13,14,13,15],[32,10,32,11],[32,13,32,15],[33,5,33,6],[33,10,33,11],[33,13,33,15],[30,10,30,11],[30,13,30,15],[31,5,31,6],[31,10,31,11],[31,13,31,15],[27,10,27,11],[28,5,28,6],[28,10,28,11],[28,13,28,15],[29,5,29,6],[29,10,29,11],[29,13,29,15],[26,13,27,15],[26,5,27,6],[26,7,26,12],[1,1,1,6],[3,1,3,15],[4,1,4,15],[5,1,5,3],[5,4,5,15],[7,1,7,6],[8,1,9,2],[8,3,9,3],[8,4,9,4],[8,5,9,5],[8,6,9,6],[8,9,9,9],[8,10,9,10],[8,11,9,11],[8,12,9,12],[8,8,9,8],[8,13,9,13],[31,2,31,3],[33,2,33,3],[10,1,16,1],[17,1,23,1],[25,1,25,6],[26,1,27,1],[26,2,27,3],[26,4,27,4],[32,2,32,3],[29,2,29,3],[30,2,30,3],[28,2,28,3],[8,7,9,7],[30,5,30,6],[32,5,32,6]]}
[]
[null,"2.5. Unit process name : Water Gas Shift reactor"]
[null,"❚Unit Process PFD"]
[null,"Unit Process PFD"]
[]
[null,"Process Description"]
[]
[null,"❚Continuous input(output) material and energy stream data",{"$nulls":9},"※For electricity, enter the kWh used per hour (kWh/hr)"]
[null,"  ",null,"Main Category","Sub-category","Origin","Input(output) name","Unit","Amount","Density\n(kg/Nm3)","LHV\n(MJ/kg)","Composition\n(mol%)","Calculation basis","Data source ","Remarks\n(For steam,\nTemp.(°C)/Press.(bar))"]
[]
[null,"Input","①","Intermediate product","Other raw materials","KOREA, REPUBLIC OF","Syngas\n[From 2.5-Out-8]","kg/hr",4900,null,null,null,"Simulation","Mass Flow Meter"]
[null,null,"②","Other by products","Heat\n(Steam, based on ~~~)","KOREA, REPUBLIC OF","Steam\n[From 2.5-Out-9]","kg/hr",10,null,null,null,"Simulation","PFD"]
[null,null,"③","Electricity","Electricity\nOther electricity","KOREA, REPUBLIC OF","Electricity\n[From 2.2-Out-11]","kWh",10000,null,null,null,"Simulation","Power Meter"]
[null,null,"④",{"$nulls":11},"  "]
[null,null,"⑤"]
[null,null,"⑥",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑦"]
[null,"Output","⑧","Intermediate product","Other raw materials","KOREA, REPUBLIC OF","Shift gas\n[To 2.7-In-1]","kg/hr",4900,null,null,null,"Simulation","Mass Flow Meter"]
[null,null,"⑨","Other by products","Other\n(Other gas fuel)","KOREA, REPUBLIC OF","Ammonia\n[To outside the system boundary]","kg/hr",60,null,null,null,"Simulation"]
[null,null,"⑩","Waste","Waste","KOREA, REPUBLIC OF","Flue gas\n[To outside the system boundary]","kg/hr",10000,null,null,null,"Simulation","Flow Meter"]
[null,null,"⑪"]
[null,null,"⑫",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑬",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑭",null,null,null,"  ","  ","  ",{"$nulls":5},"  "]
[]
[null,"❚Discontinuous input(output) stream data"]
[null,"Input\n(Output)","Main Category",null,"Sub-category","Input(Output) name",null,"Detailed Information",{"$nulls":5},"Remarks"]
[{"$nulls":7},"Annual\ninput(output) ammount","(Bulk) density","Active Ingredients","Detailed composition\n(including solvent)",null,"CAS No."]

{"sheet":"2.6. CO2 Capture","index":13,"n_rows":40,"n_cols":15,"rows_kept":40,"cut":false,"hidden":false,"merged":[[20,14,20,15],[21,14,21,15],[22,14,22,15],[23,14,23,15],[15,14,15,15],[16,14,16,15],[17,14,17,15],[18,14,18,15],[19,14,19,15],[10,14,10,15],[11,14,11,15],[12,14,12,15],[13,14,13,15],[14,14,14,15],[29,13,29,15],[30,5,30,6],[30,10,30,11],[30,13,30,15],[33,5,33,6],[33,10,33,11],[33,13,33,15],[31,5,31,6],[31,10,31,11],[31,13,31,15],[32,5,32,6],[32,10,32,11],[32,13,32,15],[7,1,7,6],[8,1,9,2],[8,3,9,3],[8,4,9,4],[8,5,9,5],[8,6,9,6],[1,1,1,6],[3,1,3,15],[4,1,4,15],[5,1,5,3],[5,4,5,15],[8,13,9,13],[8,11,9,11],[8,12,9,12],[28,2,28,3],[25,1,25,6],[26,1,27,1],[26,2,27,3],[26,4,27,4],[26,5,27,6],[26,13,27,15],[10,1,16,1],[17,1,23,1],[8,7,9,7],[26,7,26,12],[28,13,28,15],[8,14,9,15],[33,2,33,3],[35,1,35,6],[8,8,9,8],[8,9,9,9],[8,10,9,10],[32,2,32,3],[30,2,30,3],[31,2,31,3],[27,10,27,11],[28,5,28,6],[28,10,28,11],[29,2,29,3],[29,5,29,6],[29,10,29,11],[36,2,36,3],[36,7,36,15],[37,1,38,1],[37,2,38,3],[37,4,38,4],[37,5,38,5],[37,6,38,6],[37,7,38,15],[39,2,40,3],[39,4,40,4],[39,5,40,5],[39,6,40,6],[39,7,40,15]]}
[]
[null,"2.6. Unit process name : CO2 Capture"]
[null,"❚Unit Process PFD"]
[null,"Unit Process PFD"]
[]
[null,"Process Description"]
[]
[null,"❚Continuous input(output) material and energy stream data",{"$nulls":9},"※For electricity, enter the kWh used per hour (kWh/hr)"]
[null,"  ",null,"Main Category","Sub-category","Origin","Input(output) name","Unit","Amount","Density\n(kg/Nm3)","LHV\n(MJ/kg)","Composition\n(mol%)","Calculation basis","Data source ","Remarks\n(For steam,\nTemp.(°C)/Press.(bar))"]
[]
[null,"Input","①","Intermediate product","Other raw materials","KOREA, REPUBLIC OF","Shift gas\n[From 2.6-Out-8]","kg/hr",4900,{"$nulls":4},"Mass Flow Meter"]
[null,null,"②","Other raw metarial","Common\n(Industrial water)","KOREA, REPUBLIC OF","Process water\n[From outside the system boundary]","kg/hr",10000,{"$nulls":4},"PFD"]
[null,null,"③","Electricity","Electricity\nOther electricity","KOREA, REPUBLIC OF","Electricity\n[From 2.2-Out-12]","kWh",10000,{"$nulls":4},"Power Meter"]
[null,null,"④",{"$nulls":11},"  "]
[null,null,"⑤"]
[null,null,"⑥",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑦"]
[null,"Output","⑧","Intermediate product","Other raw materials","KOREA, REPUBLIC OF","Refined Gas\n[To 2.8-In-1]","kg/hr",4900,{"$nulls":4},"Mass Flow Meter"]
[null,null,"⑨","Waste","Waste","KOREA, REPUBLIC OF","~~ Gas\n[To outside the system boundary]","kg/hr",10000,{"$nulls":4},"Flow Meter"]
[null,null,"⑩","Other by products","Other\n(Other gas fuel)","KOREA, REPUBLIC OF","Ammonia\n[To outside the system boundary]","kg/hr",60]
[null,null,"⑪","Other by products","Other\n(Other gas fuel)","KOREA, REPUBLIC OF","Captured CO2\n[To 2.11-In-1]","kg/hr",60]
[null,null,"⑫",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑬",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑭",null,null,null,"  ","  ","  ",{"$nulls":5},"  "]
[]
[null,"❚Discontinuous input(output) stream data"]
[null,"Input\n(Output)","Main Category",null,"Sub-category","Input(Output) name",null,"Detailed Information",{"$nulls":5},"Remarks"]
[{"$nulls":7},"Annual\ninput(output) ammount","(Bulk) density","Active Ingredients","Detailed composition\n(including solvent)",null,"CAS No."]
{"$rows_empty":7}
[null,"❚ Purity and pressure of final captured CO2"]
[null,null,"Category-Input(Output) name",null,"Purity (Vol%)","Temperature (*C)","Pressure (bar)","Note."]
[null,null,"Captured CO2",null,0.97,null,"20 bar","CO2 Capture efficiency (95%)"]
[]
[null,null,"CO2 Compression",null,0.99,null,"20 bar"]

{"sheet":"2.7. Pressure Swing Adsorption","index":14,"n_rows":38,"n_cols":15,"rows_kept":38,"cut":false,"hidden":false,"merged":[[20,14,20,15],[21,14,21,15],[22,14,22,15],[23,14,23,15],[15,14,15,15],[16,14,16,15],[17,14,17,15],[18,14,18,15],[19,14,19,15],[10,14,10,15],[11,14,11,15],[12,14,12,15],[13,14,13,15],[14,14,14,15],[39,6,40,6],[39,7,40,15],[33,13,33,15],[28,2,28,3],[1,1,1,6],[3,1,3,15],[4,1,4,15],[37,1,38,1],[37,2,38,3],[37,4,38,5],[37,6,38,6],[37,7,38,15],[33,2,33,3],[35,1,35,6],[36,2,36,3],[36,4,36,5],[36,7,36,15],[33,5,33,6],[33,10,33,11],[29,2,29,3],[30,2,30,3],[29,5,29,6],[29,10,29,11],[29,13,29,15],[30,5,30,6],[30,10,30,11],[30,13,30,15],[32,2,32,3],[31,2,31,3],[32,5,32,6],[32,10,32,11],[32,13,32,15],[31,5,31,6],[31,10,31,11],[31,13,31,15],[26,13,27,15],[26,7,26,12],[26,5,27,6],[27,10,27,11],[28,5,28,6],[28,10,28,11],[28,13,28,15],[5,1,5,3],[5,4,5,15],[7,1,7,6],[8,1,9,2],[8,3,9,3],[8,4,9,4],[8,5,9,5],[8,6,9,6],[8,7,9,7],[8,8,9,8],[8,9,9,9],[8,10,9,10],[8,11,9,11],[8,12,9,12],[8,13,9,13],[8,14,9,15],[10,1,16,1],[17,1,23,1],[25,1,25,6],[26,1,27,1],[26,2,27,3],[26,4,27,4]]}
[]
[null,"2.7. Unit process name : Pressure Swing Adsorption (PSA)"]
[null,"❚Unit Process PFD"]
[null,"Unit Process PFD"]
[]
[null,"Process Description"]
[]
[null,"❚Continuous input(output) material and energy stream data",{"$nulls":9},"※For electricity, enter the kWh used per hour (kWh/hr)"]
[null,"  ",null,"Main Category","Sub-category","Origin","Input(output) name","Unit","Amount","Density\n(kg/Nm3)","LHV\n(MJ/kg)","Composition\n(mol%)","Calculation basis","Data source ","Remarks\n(For steam,\nTemp.(°C)/Press.(bar))"]
[]
[null,"Input","①","Intermediate product","Other raw materials","KOREA, REPUBLIC OF","Refined Gas\n(Hydrogen Purity ~%)\n[From 2.7-Out-8]","kg/hr",4900,{"$nulls":4},"Mass Flow Meter"]
[null,null,"②","Electricity","Electricity\nOther electricity","KOREA, REPUBLIC OF","Electricity\n[From 2.2-Out-13]","kWh",10000,{"$nulls":4},"Power Meter"]
[null,null,"③"]
[null,null,"④",{"$nulls":11},"  "]
[null,null,"⑤"]
[null,null,"⑥",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑦"]
[null,"Output","⑧","Output material","Hydrogen","KOREA, REPUBLIC OF","Hydrogen(Purity ~%)\n[To 2.9-In-1]","kg/hr",4900,{"$nulls":4},"Mass Flow Meter"]
[null,null,"⑨","Waste","Waste","KOREA, REPUBLIC OF","Flue gas\n[To outside the system boundary]","kg/hr",10000,{"$nulls":4},"Flow Meter"]
[null,null,"⑩"]
[null,null,"⑪"]
[null,null,"⑫",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑬",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑭",null,null,null,"  ","  ","  ",{"$nulls":5},"  "]
[]
[null,"❚Discontinuous input(output) stream data"]
[null,"Input\n(Output)","Main Category",null,"Sub-category","Input(Output) name",null,"Detailed Information",{"$nulls":5},"Remarks"]
[{"$nulls":7},"Annual\ninput(output) ammount","(Bulk) density","Active Ingredients","Detailed composition\n(including solvent)",null,"CAS No."]
{"$rows_empty":7}
[null,"❚Final product hydrogen purity and pressure"]
[null,null,"Product",null,"Purity (Vol%)",null,"Pressure (bar)","Detailed composition (Vol%)"]
[null,null,"Hydrogen",null,0.999,null,"20 bar","H2 99.9%, CO 0.05%, N2 0.05%"]

{"sheet":"2.8. Compression (If nec.)","index":15,"n_rows":38,"n_cols":15,"rows_kept":38,"cut":false,"hidden":false,"merged":[[32,13,32,15],[33,5,33,6],[33,10,33,11],[33,13,33,15],[29,13,29,15],[30,5,30,6],[30,10,30,11],[30,13,30,15],[31,5,31,6],[31,10,31,11],[31,13,31,15],[29,10,29,11],[32,10,32,11],[1,1,1,6],[3,1,3,15],[4,1,4,15],[5,1,5,3],[5,4,5,15],[7,1,7,6],[8,1,9,2],[8,3,9,3],[8,4,9,4],[8,5,9,5],[8,6,9,6],[28,2,28,3],[26,13,27,15],[26,7,26,12],[26,5,27,6],[27,10,27,11],[28,5,28,6],[28,10,28,11],[28,13,28,15],[31,2,31,3],[32,2,32,3],[29,2,29,3],[30,2,30,3],[29,5,29,6],[32,5,32,6],[8,11,9,11],[8,12,9,12],[8,13,9,13],[10,1,16,1],[8,7,9,7],[8,8,9,8],[8,9,9,9],[8,10,9,10],[8,14,9,15],[10,14,10,15],[11,14,11,15],[12,14,12,15],[13,14,13,15],[14,14,14,15],[15,14,15,15],[17,1,23,1],[25,1,25,6],[26,1,27,1],[26,2,27,3],[26,4,27,4],[21,14,21,15],[22,14,22,15],[23,14,23,15],[16,14,16,15],[17,14,17,15],[18,14,18,15],[19,14,19,15],[20,14,20,15],[39,6,40,6],[39,7,40,15],[33,2,33,3],[35,1,35,6],[36,2,36,3],[36,4,36,5],[36,7,36,15],[37,1,38,1],[37,2,38,3],[37,4,38,5],[37,6,38,6],[37,7,38,15]]}
[]
[null,"2.8. Unit process name : Hydrogen Compression"]
[null,"❚Unit Process PFD"]
[null,"Unit Process PFD"]
[]
[null,"Process Description"]
[]
[null,"❚Continuous input(output) material and energy stream data",{"$nulls":9},"※For electricity, enter the kWh used per hour (kWh/hr)"]
[null,"  ",null,"Main Category","Sub-category","Origin","Input(output) name","Unit","Amount","Density\n(kg/Nm3)","LHV\n(MJ/kg)","Composition\n(mol%)","Calculation basis","Data source ","Remarks\n(For steam,\nTemp.(°C)/Press.(bar))"]
[]
[null,"Input","①"]
[null,null,"②"]
[null,null,"③"]
[null,null,"④"]
[null,null,"⑤"]
[null,null,"⑥"]
[null,null,"⑦"]
[null,"Output","⑧"]
[null,null,"⑨"]
[null,null,"⑩"]
[null,null,"⑪"]
[null,null,"⑫",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑬",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑭",null,null,null,"  ","  ","  ",{"$nulls":5},"  "]
[]
[null,"❚Discontinuous input(output) stream data"]
[null,"Input\n(Output)","Main Category",null,"Sub-category","Input(Output) name",null,"Detailed Information",{"$nulls":5},"Remarks"]
[{"$nulls":7},"Annual\ninput(output) ammount","(Bulk) density","Active Ingredient","Detailed composition\n(including solvent)",null,"CAS No."]
{"$rows_empty":7}
[null,"❚Final product hydrogen purity and pressure"]
[null,null,"Product",null,"Purity (Vol%)",null,"Pressure (bar)","Detailed composition (Vol%)"]
[null,null,"Hydrogen",null,0.999,null,"20 bar","H2 99.9%, CO 0.05%, N2 0.05%"]

{"sheet":"2.9. Air Separation Unit","index":16,"n_rows":28,"n_cols":15,"rows_kept":28,"cut":false,"hidden":false,"merged":[[21,14,21,15],[22,14,22,15],[23,14,23,15],[16,14,16,15],[17,14,17,15],[18,14,18,15],[19,14,19,15],[20,14,20,15],[33,10,33,11],[33,13,33,15],[30,13,30,15],[31,5,31,6],[31,10,31,11],[31,13,31,15],[32,5,32,6],[32,10,32,11],[32,13,32,15],[30,5,30,6],[30,10,30,11],[1,1,1,6],[3,1,3,15],[4,1,4,15],[5,1,5,3],[5,4,5,15],[7,1,7,6],[8,1,9,2],[8,3,9,3],[8,4,9,4],[8,5,9,5],[8,6,9,6],[28,2,28,3],[26,13,27,15],[26,7,26,12],[26,5,27,6],[27,10,27,11],[28,5,28,6],[28,10,28,11],[28,13,28,15],[8,11,9,11],[8,12,9,12],[8,13,9,13],[10,1,16,1],[8,7,9,7],[8,8,9,8],[8,9,9,9],[8,10,9,10],[8,14,9,15],[10,14,10,15],[11,14,11,15],[12,14,12,15],[13,14,13,15],[14,14,14,15],[15,14,15,15],[33,2,33,3],[17,1,23,1],[25,1,25,6],[26,1,27,1],[26,2,27,3],[26,4,27,4],[31,2,31,3],[32,2,32,3],[29,2,29,3],[30,2,30,3],[29,5,29,6],[33,5,33,6],[29,10,29,11],[29,13,29,15]]}
[]
[null,"2.9. Unit process name : Air Separation Unit"]
[null,"❚Unit Process PFD"]
[null,"Unit Process PFD"]
[]
[null,"Process Description"]
[]
[null,"❚Continuous input(output) material and energy flow information",{"$nulls":9},"※For electricity, enter the kWh used per hour (kWh/hr)"]
[null,"  ",null,"Main Category","Sub-category","Origin","Input(output) name","Unit","Amount","Density\n(kg/Nm3)","LHV\n(MJ/kg)","Composition\n(mol%)","Calculation basis","Data source ","Remarks\n(For steam,\nTemp.(°C)/Press.(bar))"]
[]
[null,"Input","①","Other raw metarials","Other raw materials","KOREA, REPUBLIC OF","Air\n[From outside the system boundary]","kg/hr",100,null,null,null,"Self-calculation\nbased on\nspecification","Mass Flow Meter"]
[null,null,"②","Electricity","Grid Electricity","KOREA, REPUBLIC OF","Electricity (Grid Power)\n[From 2.2-Out-15]","kWh",10000,null,null,null,"Self-calculation\nbased on\nspecification","Power Meter"]
[null,null,"③"]
[null,null,"④"]
[null,null,"⑤"]
[null,null,"⑥",{"$nulls":5},"  "]
[null,null,"⑦"]
[null,"Output","⑧","Output materials","Hydrogen","KOREA, REPUBLIC OF","Hydrogen(Purity 99.9%)","kg/hr",4900,null,null,null,"Self-calculation\nbased on\nspecification","Mass Flow Meter"]
[null,null,"⑨"]
[null,null,"⑩"]
[null,null,"⑪"]
[null,null,"⑫",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑬",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑭",null,null,null,"  ","  ","  ",{"$nulls":5},"  "]
[]
[null,"❚Discontinuous input(output) stream data"]
[null,"Input\n(Output)","Main Category",null,"Sub-category","Input(Output) name",null,"Detailed Information",{"$nulls":5},"Remarks"]
[{"$nulls":7},"Annual\ninput(output) ammount","(Bulk) density","Effective component","Detailed composition\n(including solvent)",null,"CAS No."]

{"sheet":"2.10. CO2 Storage","index":17,"n_rows":34,"n_cols":15,"rows_kept":34,"cut":false,"hidden":false,"merged":[[30,7,30,15],[31,7,31,15],[32,7,32,15],[33,7,33,15],[11,14,11,15],[13,14,13,15],[16,14,16,15],[21,14,21,15],[20,14,20,15],[19,14,19,15],[18,14,18,15],[17,14,17,15],[10,1,17,1],[18,1,23,1],[25,1,25,6],[26,2,26,3],[1,1,1,6],[3,1,3,14],[4,1,4,14],[5,1,5,3],[7,1,7,6],[8,1,9,2],[8,3,9,3],[8,4,9,4],[8,5,9,5],[8,6,9,6],[2,4,2,8],[23,14,23,15],[33,2,33,3],[8,7,9,7],[8,8,9,8],[8,11,9,11],[8,12,9,12],[32,2,32,3],[26,7,26,15],[27,7,27,15],[28,7,28,15],[29,7,29,15],[10,14,10,15],[27,2,27,3],[12,14,12,15],[22,14,22,15],[15,14,15,15],[14,14,14,15],[5,4,5,14],[8,9,9,9],[8,10,9,10],[8,13,9,13],[8,14,9,15]]}
[]
[null,"2.10. Unit process name : CO2 Storage"]
[null,"❚Unit Process PFD",null,null,"※When including detailed processes (Liquefaction (LCO₂), Storage·Loading·Unloading, Transportation, Injection, etc.), specify each process separately."]
[null,"Unit Process PFD"]
[]
[null,"Process Description"]
[]
[null,"❚Continuous input(output) material and energy stream data",{"$nulls":9},"※For electricity, enter the kWh used per hour (kWh/hr)"]
[null,"  ",null,"Main Category","Sub-category","Origin","Input(output) name","Unit","Amount","Density\n(kg/Nm3)","LHV\n(MJ/kg)","Composition\n(mol%)","Calculation basis","Data source ","Remarks\n(For steam,\nTemp.(°C)/Press.(bar))"]
[]
[null,"Input","①","Other by-product","Other Raw Materials","KOREA, REPUBLIC OF","Sequestration CO2\n[From 2.7-Out-11]","kg/hr",60,null,null,null,"Self-calculation\nbased on\nspecification","Mass Flow Meter"]
[null,null,"②","Electricity","Grid Electricity","KOREA, REPUBLIC OF","Electricity\n(CO2 storage at the port of loading)\n[From 2.2-Out-16]","kWh",{"$nulls":4},"Self-calculation\nbased on\nspecification","Power Meter"]
[null,null,"③","Electricity","Grid Electricity","KOREA, REPUBLIC OF","Electricity\n(CO2 transportation by ship)\n[From 2.2-Out-16]","kWh",{"$nulls":4},"Self-calculation\nbased on\nspecification","Power Meter"]
[null,null,"④","Electricity","Grid Electricity","AUSTRALIA","Electricity\n(CO2 storage at the port of unloading)\n[From 2.2-Out-16]","kWh",{"$nulls":4},"Self-calculation\nbased on\nspecification","Power Meter","  "]
[null,null,"⑤","Electricity","Grid Electricity","AUSTRALIA","Electricity\n[CO2 transportation \n(Unloading port-storage)]\n[From 2.2-Out-16]","kWh",{"$nulls":4},"Self-calculation\nbased on\nspecification","Power Meter"]
[null,null,"⑥","Electricity","Grid Electricity","AUSTRALIA","Electricity\n(CO2 storage site injection)\n[From 2.2-Out-16]","kWh",{"$nulls":4},"Self-calculation\nbased on\nspecification","Power Meter","  "]
[null,null,"⑦","Fuel for other transportation facilities\n(including mobile combustion)","Other\n(Other liquid fuel)","AUSTRALIA","Fuel for transportation","kg/hr",{"$nulls":4},"Self-calculation\nbased on\nspecification","Mass Flow Meter"]
[null,null,"⑧",null,null,null,"Classification according to electricity usage required.\nEx) CO2 transprotation, \nCO2 liquefaction, CO2 storage"]
[null,"Output","⑨","Other by-product",null,"KOREA, REPUBLIC OF","Sequestered CO2\n[To outside the system boundary]","kg/hr",60,null,null,null,"Self-calculation\nbased on\nspecification","Mass Flow Meter","  "]
[null,null,"⑩","Waste","Waste","KOREA, REPUBLIC OF","CO2 loss\n[To outside the system boundary]","kg/hr",1,null,null,null,"Ex) 1% of sequestration","Mass Flow Meter","  "]
[null,null,"⑪",{"$nulls":10},"  ","  "]
[null,null,"⑫"]
[null,null,"⑬",{"$nulls":5},"  ",{"$nulls":4},"  ","  "]
[null,null,"⑭",{"$nulls":5},"  ",{"$nulls":4},"  ","  "]
[]
[null,"❚Additional information by CCS process"]
[null,"No.","Process detail",null,"Transportation distance(km)","Temperature","Pressure","Others"]
[null,1,"CO2 transportation(capture facility - storage site injection)",null,"-"]
[null,2,"CO2 storage at the port of loading"]
[null,3,"CO2 transportation by ship"]
[null,4,"CO2 storage at the port of unloading"]
[null,5,"CO2 transportation(Unloading port-storage)"]
[null,6,"CO2 storage site injection",null,"-",null,null,"ex1) Storage Amount = Injection Amount * Injection Leakage Rate\nex2) Storage Amount = Captured Amount * Leakage Rate per CCS Process"]
[null,7]

{"sheet":"2.11. Ind.&WasteTreat.(If nec.)","index":18,"n_rows":28,"n_cols":15,"rows_kept":28,"cut":false,"hidden":false,"merged":[[22,14,22,15],[23,14,23,15],[17,14,17,15],[18,14,18,15],[19,14,19,15],[20,14,20,15],[21,14,21,15],[32,10,32,11],[32,13,32,15],[33,5,33,6],[33,10,33,11],[33,13,33,15],[30,10,30,11],[30,13,30,15],[31,5,31,6],[31,10,31,11],[31,13,31,15],[28,5,28,6],[28,10,28,11],[28,13,28,15],[29,5,29,6],[29,10,29,11],[29,13,29,15],[3,1,3,15],[4,1,4,15],[5,1,5,3],[5,4,5,15],[27,10,27,11],[26,13,27,15],[26,5,27,6],[26,7,26,12],[8,14,9,15],[10,14,10,15],[11,14,11,15],[12,14,12,15],[13,14,13,15],[14,14,14,15],[15,14,15,15],[16,14,16,15],[7,1,7,6],[8,1,9,2],[8,3,9,3],[8,4,9,4],[8,5,9,5],[8,6,9,6],[8,9,9,9],[8,10,9,10],[8,11,9,11],[8,12,9,12],[8,8,9,8],[8,13,9,13],[31,2,31,3],[33,2,33,3],[10,1,16,1],[17,1,23,1],[25,1,25,6],[26,1,27,1],[26,2,27,3],[26,4,27,4],[32,2,32,3],[29,2,29,3],[30,2,30,3],[28,2,28,3],[8,7,9,7],[30,5,30,6],[32,5,32,6]]}
[]
[null,"2.11. Unit process name : Industrial Water & Wastewater Treatment_(If necessary)"]
[null,"❚Unit Process PFD"]
[null,"Unit Process PFD"]
[]
[null,"Process Description"]
[]
[null,"❚Continuous input(output) material and energy stream data",{"$nulls":9},"※For electricity, enter the kWh used per hour (kWh/hr)"]
[null,"  ",null,"Main Category","Sub-category","Origin","Input(output) name","Unit","Amount","Density\n(kg/Nm3)","LHV\n(MJ/kg)","Composition\n(mol%)","Calculation basis","Data source ","Remarks\n(For steam,\nTemp.(°C)/Press.(bar))"]
[]
[null,"Input","①"]
[null,null,"②"]
[null,null,"③"]
[null,null,"④"]
[null,null,"⑤"]
[null,null,"⑥"]
[null,null,"⑦"]
[null,"Output","⑧"]
[null,null,"⑨"]
[null,null,"⑩"]
[null,null,"⑪"]
[null,null,"⑫",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑬",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑭",null,null,null,"  ","  ","  ",{"$nulls":5},"  "]
[]
[null,"❚Discontinuous input(output) stream data"]
[null,"Input\n(Output)","Main Category",null,"Sub-category","Input(Output) name",null,"Detailed Information",{"$nulls":5},"Remarks"]
[{"$nulls":7},"Annual\ninput(output) ammount","(Bulk) density","Active Ingredient","Detailed composition\n(including solvent)",null,"CAS No."]

{"sheet":"2.12. Other Utilities(If nec.)","index":19,"n_rows":28,"n_cols":15,"rows_kept":28,"cut":false,"hidden":false,"merged":[[19,14,19,15],[20,14,20,15],[21,14,21,15],[22,14,22,15],[23,14,23,15],[14,14,14,15],[15,14,15,15],[16,14,16,15],[17,14,17,15],[18,14,18,15],[8,14,9,15],[10,14,10,15],[11,14,11,15],[12,14,12,15],[13,14,13,15],[32,10,32,11],[32,13,32,15],[33,5,33,6],[33,10,33,11],[33,13,33,15],[30,10,30,11],[30,13,30,15],[31,5,31,6],[31,10,31,11],[31,13,31,15],[27,10,27,11],[28,5,28,6],[28,10,28,11],[28,13,28,15],[29,5,29,6],[29,10,29,11],[29,13,29,15],[26,13,27,15],[26,5,27,6],[26,7,26,12],[1,1,1,6],[3,1,3,15],[4,1,4,15],[5,1,5,3],[5,4,5,15],[7,1,7,6],[8,1,9,2],[8,3,9,3],[8,4,9,4],[8,5,9,5],[8,6,9,6],[8,9,9,9],[8,10,9,10],[8,11,9,11],[8,12,9,12],[8,8,9,8],[8,13,9,13],[31,2,31,3],[33,2,33,3],[10,1,16,1],[17,1,23,1],[25,1,25,6],[26,1,27,1],[26,2,27,3],[26,4,27,4],[32,2,32,3],[29,2,29,3],[30,2,30,3],[28,2,28,3],[8,7,9,7],[30,5,30,6],[32,5,32,6]]}
[]
[null,"2.12. Unit process name : Other utility(If necessary)"]
[null,"❚Unit Process PFD"]
[null,"Unit Process PFD"]
[]
[null,"Process Description"]
[]
[null,"❚Continuous input(output) material and energy stream data",{"$nulls":9},"※For electricity, enter the kWh used per hour (kWh/hr)"]
[null,"  ",null,"Main Category","Sub-category","Origin","Input(output) name","Unit","Amount","Density\n(kg/Nm3)","LHV\n(MJ/kg)","Composition\n(mol%)","Calculation basis","Data source ","Remarks\n(For steam,\nTemp.(°C)/Press.(bar))"]
[]
[null,"Input","①"]
[null,null,"②"]
[null,null,"③"]
[null,null,"④"]
[null,null,"⑤"]
[null,null,"⑥"]
[null,null,"⑦"]
[null,"Output","⑧"]
[null,null,"⑨"]
[null,null,"⑩"]
[null,null,"⑪"]
[null,null,"⑫",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑬",{"$nulls":5},"  ",{"$nulls":5},"  "]
[null,null,"⑭",null,null,null,"  ","  ","  ",{"$nulls":5},"  "]
[]
[null,"❚Discontinuous input(output) stream data"]
[null,"Input\n(Output)","Main Category",null,"Sub-category","Input(Output) name",null,"Detailed Information",{"$nulls":5},"Remarks"]
[{"$nulls":7},"Annual\ninput(output) ammount","(Bulk) density","Active Ingredients","Detailed composition\n(including solvent)",null,"CAS No."]

{"sheet":"3. Operating Conditions & Plan","index":20,"n_rows":32,"n_cols":14,"rows_kept":32,"cut":false,"hidden":false,"merged":[[2,1,2,12],[13,2,13,10],[13,11,13,16],[8,1,8,16],[7,1,7,16],[10,11,10,16]]}
[]
[]
[null,"3. Operating Condition and Production Plan"]
[]
[]
[null,"❚Overall process"]
[]
[null,"Overall process"]
[]
[]
[null,"❚Monthly Input/Output Quantities of Hydrogen Production",{"$nulls":9},"※ Target for Documentation: Mass and energy flows that enter and exit the system boundary amont \nthe unit process material flows in sheet 2.X"]
[{"$nulls":11},"※ Note: Consider the number of days per month and the operating rate"]
[]
[null,null,"Input",{"$nulls":8},"Output"]
[null,"Main Category","Raw material","Fuel","Fuel","Electricity","Electricity","Electricity","Steam","Fuel",null,"Output\nmaterial","Output\nmaterial","Waste"]
[null,"sub-category","Common\n(Industrial water)","Chemical substance\n(HCI solution)","Chemical substance\n(NaOH solution)","Electricity\n(Renewable Enegy-Solar)","Electricity\n(Renewable Enegy-Grid)","Electricity\n(Renewable Enegy-Wind)","Heat\n(based on fuel)","Natural Gas\n(Domestic city gas)",null,"Hydrogen","Chemical substance\n(Oxygen)","Waste"]
[null,"Data source ","PFD","PFD","PFD","PFD","PFD","PFD","PFD","PFD",null,"PFD","PFD","PFD"]
[null,"Origin","Within System Boundary","Within System Boundary","Within System Boundary","Within System Boundary","Within System Boundary","Within System Boundary","Within System Boundary","Within System Boundary",null,"Within System Boundary","Within System Boundary","Within System Boundary"]
[null,"           Unit\nPeriod","kg","kg","kg","kWh","kWh","kWh","kg","kg",null,"kg","kg","kg"]
[null,"Jan",369383.75,1.2830872727272729,3.0367527272727277,1846800,68400,136800,660850,1000,null,39719.879999999997,301871.08799999999,4.319840000000001]
[null,"Feb",365284,1.2961800000000001,3.0677400000000001,1827360,67680,135360,660850,1000,null,39301.775999999998,295549.35551999998,4.3639200000000002]
[null,"Mar",360933,1.3292563636363635,3.1460236363636365,1807920,66960,133920,660850,1000,null,38883.672000000006,289294.51968000008,4.4752799999999997]
[null,"Apr",357328,1.3471727272727274,3.1884272727272731,1788480,66240,132480,660850,1000,null,38465.568000000007,283106.58048000006,4.5356000000000005]
[null,"May",352898,1.3471727272727301,3.1884272727272731,1769040,65520,131040,660850,1000,null,38047.464,276985.53792000003,4.5356000000000032]
[null,"Jun",347400,1.3526854545454543,3.2014745454545452,1749600,64800,129600,660850,1000,null,37629.360000000001,270931.39199999999,4.5541599999999995]
[null,"Jul",369360,1.3595763636363636,3.2177836363636363,1846800,68400,136800,660850,1000,null,39719.879999999997,301871.08799999999,4.5773599999999997]
[null,"Aug",365472,1.3471727272727274,3.1884272727272731,1827360,67680,135360,660850,1000,null,39301.775999999998,295549.35551999998,4.5356000000000005]
[null,"Sep",373248,1.3451054545454544,3.1835345454545454,1866240,69120,138240,660850,1000,null,40137.983999999997,308259.71711999999,4.5286399999999993]
[null,"Oct",377136,1.320298181818182,3.124821818181819,1885680,69840,139680,660850,1000,null,40556.088000000003,314715.24288000003,4.4451200000000011]
[null,"Nov",369360,1.305138181818182,3.0889418181818189,1846800,68400,136800,660850,1000,null,39719.879999999997,301871.08799999999,4.3940800000000007]
[null,"Dec",365472,1.2851545454545457,3.0416454545454554,1827360,67680,135360,660850,1000,null,39301.775999999998,295549.35551999998,4.3268000000000013]
[null,"Sum",{"$f":"SUM(C20:C31)","v":4373274.75},{"$f":"SUM(D20:D31)","v":15.918000000000005},{"$f":"SUM(E20:E31)","v":37.673999999999999},{"$f":"SUM(F20:F31)","v":21889440},{"$f":"SUM(G20:G31)","v":810720},{"$f":"SUM(H20:H31)","v":1621440},{"$f":"SUM(I20:I31)","v":7930200},12000,null,{"$f":"SUM(L20:L31)","v":470785.10400000005},{"$f":"SUM(M20:M31)","v":3535554.3206400005},{"$f":"SUM(N20:N31)","v":53.592000000000006}]

{"sheet":"4. Disclaimer","index":21,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[[1,1,27,11]]}

{"sheet":"Q&A","index":22,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[[1,1,27,11]]}

{"sheet":"Ecoinvent Index Method","index":23,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[[18,6,20,10]]}
[]
[null,"1. Access the site(https://ecoquery.ecoinvent.org/3.9.1/cutoff/search)"]
[]
[{"$nulls":6},"Select of the Release 3.9.1, Allocation, cut-off by classification"]
[]
[]
[]
[]
[{"$nulls":6},"Search the material name"]
[]
[{"$nulls":6},"Check the description of the material"]
[]
[]
[]
[]
[null,"2. Check the \"Details\" of the material description and write down the Activity Name and Geography"]
[]
[]
[{"$nulls":6},"Directly review the description and find the relevant substance or the substance most similar to it, and then submit"]

{"sheet":"데이터 코드 ","index":24,"n_rows":323,"n_cols":5,"rows_kept":323,"cut":false,"hidden":true,"merged":[]}
[]
[]
[null,null,"투입-산출물 데이터 코드 (AA - BBBB - CC)"]
[null,null,"AA: 데이터 대분류, BBBB: 데이터 중분류 및 세분류, CC: 원산지 국가 코드"]
[null,null,"<예시>"]
[null,null,"예시 1: (F0-0001-ZZ) : 한국 연료용 도시가스"]
[null,null,"예시 2: (R1-0012-AU) : 호주산 원료용 유연탄"]
[null,null,"예시 3: (R1-0002-MY) : 말레이시아산 원료용 천연가스 (한국 사용)"]
[null,null,"예시 4: (R1-0004-US) : 미국산 원료용 천연가스 (미국 사용)"]
[null,null,"예시 5: (P1-0000-ZZ) : 최종 제품 수소"]
[null,null,"예시 6: (E0-0081-AU) : 호주 그리드 전기"]
[null,null,"예시 7: (E0-0084-KR) : 한국 수력 전기"]
[]
[null,null,"AA : <데이터 대분류>"]
[null,null,"구분","코드","활동자료 대분류명"]
[null,null,"연료","F0","수소 원료 생산 시설용 연료 (예. 초순수 제조 시설)"]
[null,null,null,"F1","수소 생산 시설용 주 연료 (예. 수증기 개질 반응기 천연가스)"]
[null,null,null,"F2","수소 생산 시설용 보조 연료"]
[null,null,null,"F3","발전 시설용 연료"]
[null,null,null,"F4","열 생산 시설용 연료"]
[null,null,null,"F5","기타 유틸리티 시설용 연료"]
[null,null,null,"F6","기타 수송 시설용 (이동 연소 포함) 연료"]
[null,null,null,"F9","기타 연료"]
[null,null,"원료","R1","수소 생산 원료"]
[null,null,null,"R2","수소 외 제품 생산 원료"]
[null,null,null,"R3","촉매"]
[null,null,null,"R4","환원제"]
[null,null,null,"R9","기타 원료"]
[null,null,"생산물","P0","수소"]
[null,null,null,"P1","최종생산물"]
[null,null,null,"P2","중간생산물"]
[null,null,null,"P3","기타 부산물"]
[null,null,"열/전기","S0","열"]
[null,null,null,"E0","전기"]
[null,null,null,"E1","기타 전기"]
[null,null,"폐기물","W0","폐기물"]
[null,null,"기타","O0","기타 부산물"]
[]
[null,null,"BBBB : <데이터 중분류 및 세분류>"]
[null,null,"중분류명","코드","세분류명"]
[null,null,"수소","0000","수소"]
[null,null,"천연가스","0001","국내 도시가스"]
[null,null,null,"0002","수입 천연가스"]
[null,null,null,"0003","해외 도시가스"]
[null,null,null,"0004","해외 천연가스"]
[null,null,"유연탄","0011","국내 유연탄"]
[null,null,null,"0012","수입 유연탄"]
[null,null,"무연탄","0021","국내 무연탄"]
[null,null,null,"0022","수입 무연탄"]
[null,null,"액화석유가스","0031","액화석유가스"]
[null,null,"프로판","0041","프로판"]
[null,null,"중유","0051","B-C유"]
[null,null,"경유","0061","경유"]
[null,null,"휘발유","0071","휘발유"]
[null,null,"전기","0081","그리드 전기"]
[null,null,null,"0082","재생 (태양광) 전기"]
[null,null,null,"0083","재생 (풍력) 전기"]
[null,null,null,"0084","재생 (수력) 전기"]
[null,null,null,"0085","원자력 전기"]
[null,null,null,"0086","기타 전기"]
[null,null,"열","0091","열 (스팀)"]
[null,null,null,"0092","열 (온수)"]
[null,null,"공통",1001,"순수"]
[null,null,null,"1002","공업용수"]
[null,null,"기초화학물질","2001","염화수소 (HCl) 용액"]
[null,null,null,"2002","수산화나트륨 (NaOH) 용액"]
[null,null,null,"2003","이산화탄소 흡착제 (MEA)"]
[null,null,"폐기물","3001","폐수"]
[null,null,null,"3002","폐기물"]
[null,null,"기타","9001","기타 고체연료"]
[null,null,null,"9002","기타 액체연료"]
[null,null,null,"9003","기타 기체연료"]
[null,null,null,"9004","기타 원료"]
[null,null,null,"9005","산소"]
[]
[null,null,"CC: <원산지 국가코드>"]
[null,null,"국가명","코드","영문명"]
[null,null,"해당 사항 없음","ZZ","N/A"]
[null,null,"가나","GH","GHANA"]
[null,null,"가봉","GA","GABON"]
[null,null,"가이아나","GY","GUYANA"]
[null,null,"감비아","GM","GAMBIA"]
[null,null,"건지 섬","GG","GUERNSEY"]
[null,null,"과들루프","GP","GUADELOUPE"]
[null,null,"과테말라","GT","GUATEMALA"]
[null,null,"괌","GU","GUAM"]
[null,null,"그레나다","GD","GRENADA"]
[null,null,"그리스","GR","GREECE"]
[null,null,"그린란드","GL","GREENLAND"]
[null,null,"기니","GN","GUINEA"]
[null,null,"기니비사우","GW","GUINEA-BISSAU"]
[null,null,"나미비아","NA","NAMIBIA"]
[null,null,"나우루","NR","NAURU"]
[null,null,"나이지리아","NG","NIGERIA"]
[null,null,"남극","AQ","ANTARCTICA"]
[null,null,"남수단","SS","REPUBLIC OF SOUTH SUDAN"]
[null,null,"남아프리카 공화국","ZA","SOUTH AFRICA"]
[null,null,"네덜란드","NL","NETHERLANDS"]
[null,null,"네덜란드령 안틸레스","AN","NETHERLANDS ANTILLES"]
[null,null,"네팔","NP","NEPAL"]
[null,null,"노르웨이","NO","NORWAY"]
[null,null,"노퍽 섬","NF","NORFOLK ISLAND"]
[null,null,"누벨칼레도니","NC","NEW CALEDONIA"]
[null,null,"뉴질랜드","NZ","NEW ZEALAND"]
[null,null,"니우에","NU","NIUE"]
[null,null,"니제르","NE","NIGER"]
[null,null,"니카라과","NI","NICARAGUA"]
[null,null,"대한민국","KR","KOREA, REPUBLIC OF"]
[null,null,"덴마크","DK","DENMARK"]
[null,null,"도미니카 공화국","DO","DOMINICAN REPUBLIC"]
[null,null,"도미니카 연방","DM","DOMINICA"]
[null,null,"독일","DE","GERMANY"]
[null,null,"동티모르","TL","EAST TIMOR"]
[null,null,"라오스","LA","LAO PEOPLE'S DEMOCRATIC REPUBLIC"]
[null,null,"라이베리아","LR","LIBERIA"]
[null,null,"라트비아","LV","LATVIA"]
[null,null,"러시아","RU","RUSSIAN FEDERATION"]
[null,null,"레바논","LB","LEBANON"]
[null,null,"레소토","LS","LESOTHO"]
[null,null,"레위니옹","RE","REUNION"]
[null,null,"루마니아","RO","ROMANIA"]
[null,null,"룩셈부르크","LU","LUXEMBOURG"]
[null,null,"르완다","RW","RWANDA"]
[null,null,"리비아","LY","LIBYAN ARAB JAMAHIRIYA"]
[null,null,"리투아니아","LT","LITHUANIA"]
[null,null,"리히텐슈타인","LI","LIECHTENSTEIN"]
[null,null,"마다가스카르","MG","MADAGASCAR"]
[null,null,"마르티니크","MQ","MARTINIQUE"]
[null,null,"마셜 제도","MH","MARSHALL ISLANDS"]
[null,null,"마요트","YT","MAYOTTE"]
[null,null,"마카오","MO","MACAU"]
[null,null,"마케도니아 공화국","MK","REPUBLIC OF MACEDONIA"]
[null,null,"말라위","MW","MALAWI"]
[null,null,"말레이시아","MY","MALAYSIA"]
[null,null,"말리","ML","MALI"]
[null,null,"맨 섬","IM","ISLE OF MAN"]
[null,null,"멕시코","MX","MEXICO"]
[null,null,"모나코","MC","MONACO"]
[null,null,"모로코","MA","MOROCCO"]
[null,null,"모리셔스","MU","MAURITIUS"]
[null,null,"모리타니","MR","MAURITANIA"]
[null,null,"모잠비크","MZ","MOZAMBIQUE"]
[null,null,"몬테네그로","ME","MONTENEGRO"]
[null,null,"몬트세랫","MS","MONTSERRAT"]
[null,null,"몰도바","MD","MOLDOVA, REPUBLIC OF"]
[null,null,"몰디브","MV","MALDIVES"]
[null,null,"몰타","MT","MALTA"]
[null,null,"몽골","MN","MONGOLIA"]
[null,null,"미국","US","UNITED STATES"]
[null,null,"미국령 군소 제도","UM","UNITED STATES MINOR OUTLYING ISLANDS"]
[null,null,"미국령 버진아일랜드","VI","VIRGIN ISLANDS, U.S."]
[null,null,"미얀마","MM","MYANMAR"]
[null,null,"미크로네시아 연방","FM","MICRONESIA"]
[null,null,"바누아투","VU","VANUATU"]
[null,null,"바레인","BH","BAHRAIN"]
[null,null,"바베이도스","BB","BARBADOS"]
[null,null,"바티칸 시국","VA","VATICAN CITY STATE"]
[null,null,"바하마","BS","BAHAMAS"]
[null,null,"방글라데시","BD","BANGLADESH"]
[null,null,"버뮤다","BM","BERMUDA"]
[null,null,"베냉","BJ","BENIN"]
[null,null,"베네수엘라","VE","VENEZUELA"]
[null,null,"베트남","VN","VIET NAM"]
[null,null,"벨기에","BE","BELGIUM"]
[null,null,"벨라루스","BY","BELARUS"]
[null,null,"벨리즈","BZ","BELIZE"]
[null,null,"보스니아 헤르체고비나","BA","BOSNIA HERCEGOVINA"]
[null,null,"보츠와나","BW","BOTSWANA"]
[null,null,"볼리비아","BO","BOLIVIA"]
[null,null,"부룬디","BI","BURUNDI"]
[null,null,"부르키나파소","BF","BURKINA FASO"]
[null,null,"부베 섬","BV","BOUVET ISLAND"]
[null,null,"부탄","BT","BHUTAN"]
[null,null,"북마리아나 제도","MP","NORTHERN MARIANA ISLANDS"]
[null,null,"불가리아","BG","BULGARIA"]
[null,null,"브라질","BR","BRAZIL"]
[null,null,"브루나이","BN","BRUNEI DARUSSALAM"]
[null,null,"사모아","WS","SAMOA"]
[null,null,"사우디아라비아","SA","SAUDI ARABIA"]
[null,null,"사우스조지아 사우스샌드위치 제도","GS","SOUTH GEORGIA AND THE SOUTH SANDWICH ISLANDS"]
[null,null,"산마리노","SM","SAN MARINO"]
[null,null,"상투메 프린시페","ST","SAO TOME AND PRINCIPE"]
[null,null,"생피에르 미클롱","PM","ST. PIERRE AND MIQUELON"]
[null,null,"서사하라","EH","WESTERN SAHARA"]
[null,null,"세네갈","SN","SENEGAL"]
[null,null,"세르비아","RS","SERBIA"]
[null,null,"세이셸","SC","SEYCHELLES"]
[null,null,"세인트루시아","LC","SAINT LUCIA"]
[null,null,"세인트빈센트 그레나딘","VC","SAINT VINCENT AND THE GRENADINES"]
[null,null,"세인트키츠 네비스","KN","SAINT KITTS AND NEVIS"]
[null,null,"세인트헬레나","SH","ST. HELENA"]
[null,null,"소말리아","SO","SOMALIA"]
[null,null,"솔로몬 제도","SB","SOLOMON ISLANDS"]
[null,null,"수단","SD","SUDAN"]
[null,null,"수리남","SR","SURINAME"]
[null,null,"스리랑카","LK","SRI LANKA"]
[null,null,"스발바르 얀마옌","SJ","SVALBARD AND JAN MAYEN ISLANDS"]
[null,null,"스와질란드","SZ","SWAZILAND"]
[null,null,"스웨덴","SE","SWEDEN"]
[null,null,"스위스","CH","SWITZERLAND"]
[null,null,"스페인","ES","SPAIN"]
[null,null,"슬로바키아","SK","SLOVAKIA"]
[null,null,"슬로베니아","SI","SLOVENIA"]
[null,null,"시리아","SY","SYRIAN ARAB REPUBLIC"]
[null,null,"시에라리온","SL","SIERRA LEONE"]
[null,null,"싱가포르","SG","SINGAPORE"]
[null,null,"아랍에미리트","AE","ARAB EMIRATES"]
[null,null,"아루바","AW","ARUBA"]
[null,null,"아르메니아","AM","ARMENIA"]
[null,null,"아르헨티나","AR","ARGENTINA"]
[null,null,"아메리칸사모아","AS","AMERICAN SAMOA"]
[null,null,"아이슬란드","IS","ICELAND"]
[null,null,"아이티","HT","HAITI"]
[null,null,"아일랜드","IE","IRELAND"]
[null,null,"아제르바이잔","AZ","AZERBAIJAN"]
[null,null,"아프가니스탄","AF","AFGHANISTAN"]
[null,null,"안도라","AD","ANDORRA"]
[null,null,"알바니아","AL","ALBANIA"]
[null,null,"알제리","DZ","ALGERIA"]
[null,null,"앙골라","AO","ANGOLA"]
[null,null,"앤티가 바부다","AG","ANTIGUA AND BARBUDA"]
[null,null,"앵귈라","AI","ANGUILLA"]
[null,null,"에리트레아","ER","ERITREA"]
[null,null,"에스토니아","EE","ESTONIA"]
[null,null,"에콰도르","EC","ECUADOR"]
[null,null,"에티오피아","ET","ETHIOPIA"]
[null,null,"엘살바도르","SV","EL SALVADOR"]
[null,null,"영국","GB","UNITED KINGDOM"]
[null,null,"영국령 버진아일랜드","VG","VIRGIN ISLANDS, BRITISH"]
[null,null,"영국령 인도양 지역","IO","BRITISH INDIAN OCEAN TERRITORY"]
[null,null,"예멘","YE","YEMEN, REPUBLIC OF"]
[null,null,"오만","OM","OMAN"]
[null,null,"오스트레일리아","AU","AUSTRALIA"]
[null,null,"오스트리아","AT","AUSTRIA"]
[null,null,"온두라스","HN","HONDURAS"]
[null,null,"올란드 제도","AX","ALAND ISLANDS"]
[null,null,"왈리스 퓌튀나","WF","WALLIS AND FUTUNA ISLANDS"]
[null,null,"요르단","JO","JORDAN"]
[null,null,"우간다","UG","UGANDA"]
[null,null,"우루과이","UY","URUGUAY"]
[null,null,"우즈베키스탄","UZ","UZBEKISTAN"]
[null,null,"우크라이나","UA","UKRAINE"]
[null,null,"이라크","IQ","IRAQ"]
[null,null,"이란","IR","IRAN"]
[null,null,"이스라엘","IL","ISRAEL"]
[null,null,"이집트","EG","EGYPT"]
[null,null,"이탈리아","IT","ITALY"]
[null,null,"인도","IN","INDIA"]
[null,null,"인도네시아","ID","INDONESIA"]
[null,null,"일본","JP","JAPAN"]
[null,null,"자메이카","JM","JAMAICA"]
[null,null,"잠비아","ZM","ZAMBIA"]
[null,null,"저지 섬","JE","JERSEY"]
[null,null,"적도 기니","GQ","EQUATORIAL GUINEA"]
[null,null,"조선민주주의인민공화국","KP","KOREA, DEMOCRATIC PEOPLE'S REPUBLIC OF"]
[null,null,"조지아","GE","GEORGIA"]
[null,null,"중앙아프리카 공화국","CF","CENTRAL AFRICAN REPUBLIC"]
[null,null,"중화민국","TW","TAIWAN, PROVINCE OF CHINA"]
[null,null,"중화인민공화국","CN","CHINA"]
[null,null,"지부티","DJ","DJIBOUTI"]
[null,null,"지브롤터","GI","GIBRALTAR"]
[null,null,"짐바브웨","ZW","ZIMBABWE"]
[null,null,"차드","TD","CHAD"]
[null,null,"체코","CZ","CZECH REPUBLIC"]
[null,null,"칠레","CL","CHILE"]
[null,null,"카메룬","CM","CAMEROON"]
[null,null,"카보베르데","CV","CAPE VERDE"]
[null,null,"카자흐스탄","KZ","KAZAKHSTAN"]
[null,null,"카타르","QA","QATAR"]
[null,null,"캄보디아","KH","CAMBODIA"]
[null,null,"캐나다","CA","CANADA"]
[null,null,"케냐","KE","KENYA"]
[null,null,"케이맨 제도","KY","CAYMAN ISLANDS"]
[null,null,"코모로","KM","COMOROS"]
[null,null,"코스타리카","CR","COSTA RICA"]
[null,null,"코코스 제도","CC","COCOS ISLANDS"]
[null,null,"코트디부아르","CI","COTE D'IVOIRE"]
[null,null,"콜롬비아","CO","COLOMBIA"]
[null,null,"콩고 공화국","CG","CONGO"]
[null,null,"콩고 민주 공화국","CD","DEMOCRATIC REPUBLIC OF THE CONGO"]
[null,null,"쿠바","CU","CUBA"]
[null,null,"쿠웨이트","KW","KUWAIT"]
[null,null,"쿡 제도","CK","COOK ISLANDS"]
[null,null,"크로아티아","HR","CROATIA"]
[null,null,"크리스마스 섬","CX","CHRISTMAS ISLAND"]
[null,null,"키르기스스탄","KG","KYRGYZSTAN"]
[null,null,"키리바시","KI","KIRIBATI"]
[null,null,"키프로스","CY","CYPRUS"]
[null,null,"타이","TH","THAILAND"]
[null,null,"타지키스탄","TJ","TAJIKISTAN"]
[null,null,"탄자니아","TZ","TANZANIA, UNITED REPUBLIC OF"]
[null,null,"터크스 케이커스 제도","TC","TURKS AND CAICOS ISLANDS"]
[null,null,"터키","TR","TURKEY"]
[null,null,"토고","TG","TOGO"]
[null,null,"토켈라우","TK","TOKELAU"]
[null,null,"통가","TO","TONGA"]
[null,null,"투르크메니스탄","TM","TURKMENISTAN"]
[null,null,"투발루","TV","TUVALU"]
[null,null,"튀니지","TN","TUNISIA"]
[null,null,"트리니다드 토바고","TT","TRINIDAD AND TOBAGO"]
[null,null,"파나마","PA","PANAMA"]
[null,null,"파라과이","PY","PARAGUAY"]
[null,null,"파키스탄","PK","PAKISTAN"]
[null,null,"파푸아 뉴기니","PG","PAPUA NEW GUINEA"]
[null,null,"팔라우","PW","PALAU"]
[null,null,"팔레스타인","PS","PALESTINE"]
[null,null,"페로 제도","FO","FAROE ISLANDS"]
[null,null,"페루","PE","PERU"]
[null,null,"포르투갈","PT","PORTUGAL"]
[null,null,"포클랜드 제도","FK","FALKLAND ISLANDS"]
[null,null,"폴란드","PL","POLAND"]
[null,null,"푸에르토리코","PR","PUERTO RICO"]
[null,null,"프랑스","FR","FRANCE"]
[null,null,"프랑스령 기아나","GF","FRENCH GUIANA"]
[null,null,"프랑스령 남부와 남극 지역","TF","FRENCH SOUTHERN TERRITORIES"]
[null,null,"프랑스령 폴리네시아","PF","FRENCH POLYNESIA"]
[null,null,"피지","FJ","FIJI"]
[null,null,"핀란드","FI","FINLAND"]
[null,null,"필리핀","PH","PHILIPPINES"]
[null,null,"핏케언 제도","PN","PITCAIRN"]
[null,null,"허드 맥도널드 제도","HM","HEARD AND MC DONALD ISLANDS"]
[null,null,"헝가리","HU","HUNGARY"]
[null,null,"홍콩","HK","HONG KONG"]